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Checklist Number:                        OPS-TCFOI-422                                                       
Checklist Name:             OPS – Ramp Inspection                                                                                                                                                   
Applicability:                                                                                          
Location:                                                 Date:                                       





	No
	Subject
	Reference
	S
	U
	N/A
	Comment

	1
	Flight Crew Compartment

	1.1
	General Condition
• Cleanliness or hazards associated with impeded or slowed evacuations 
• Stowage of interior equipment, suitcases, navigation chart cases, EFB if applicable, etc;
• Condition of the flight deck windows (e.g. windshield cracks, possible delamination);
• No equipment is installed such that it obviously does not meet the systems design features and emergency landing provisions in applicable airworthiness requirements (e.g. when equipment installed on the glare shield significantly impairs the pilot´s vision);
• Presence and serviceability of the windshield wipers (if required for the flight);
• Serviceability of the warning panel lights;
• Inappropriate pulled circuit breakers (CB’s);
• If any electrical cables/wires are unintentionally exposed; and
• Door locking/unlocking mechanism and Crew Only placard, if reinforced flight crew compartment door is installed.
	CAT.IDE.A.250
CAT.IDE.A.285
CAT.IDE.A.100
ORO.SEC.100 (a)(b)
	
	
	
	




	1.2
	Emergency Exit
Aeroplanes required to have a separate emergency exit for the flight crew for which the lowest point of the emergency exit is more than 1,83 m (6 ft) above the ground shall have a means to assist all flight crew members in descending to reach the ground safely in an emergency.
	CAT.IDE.A.265
	
	
	
	

	1.3
	Equipment
(e.g. TAWS, EGPWS, ACAS, CVR, FDR, EFB, PA system, 8.33 kHz (if required))
General note: while checking this inspection item, should also assess whether the required equipment is obviously not being used, e.g. if an equipment is found to be covered and therefore rendered unusable, this should result in a CAT 1 finding. If equipment is found to be obstructed (e.g. by a manual) during flight preparation phase, this should not lead to a finding
	CAT.IDE.A.105
CAT.IDE.A.150, CAT.IDE.A.155, CAT.IDE.A.160
CAT.IDE.A.180 
CAT.IDE.A.185, CAT.IDE.A.190
CAT.OP.MPA.
215
CAT.IDE.A.345
CAT.IDE.A.355
CAT.GEN.MPA.141
	
	
	
	

	1.4
	Manuals
Operations Manuals and the aircraft flight manual (AFM), or equivalent document(s). 
Note: check full requirement & AMC for complete details
	CAT.GEN.MPA.180,
ORO.MLR.100
ORO.MLR.105
CAT.GEN.MPA.200 
AMC1 CAT.GEN.MPA.180(a) 
GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.5
	Checklists (Normal, Non-Normal, Emergency)
	ORO.GEN.110
(h)
CAT.GEN.MPA.180,
AMC1 CAT.GEN.MPA.180(a) 
GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.6
	Navigation Charts 
• Validity of the FMS/GPS database
• Required charts availability:
· en-route, departure, approach and aerodrome;
· within reach;
· up to date to the latest AIRAC amendments;
including those for the alternate aerodromes
	CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
CAT.IDE.A.355

	
	
	
	

	1.7
	Original Certificate of Registration
• The presence and accuracy;
• If the format and content are in accordance with the requirements; and
• If there is a translation into the English language.


	CAT.GEN.MPA.180
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.8
	Original Certificate of Airworthiness 
(C of A)
• Presence, accuracy and validity.
• If the content is in compliance with the requirement (including English translation if written in another language).
	CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.9
	Noise Certificate (if applicable)
• Presence, accuracy (e.g. cross check MTOM, S/N with the ones specified in the C of R) of the document attesting noise certification, as original or copy; and
• Whether it is translated in English language (translation provided by the authority responsible for issuing the noise certificate).
	CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.10
	Original / Certified true copy of the AOC
	CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.11
	Operations Specifications Relevant to the aircraft type
	CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.12
	Original Radio Licence (if applicable)
• Presence, accuracy of the information mentioned on the Radio Station Licence
 (if available);
• The correct name/callsign.
	CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.13
	Third-Party Liability Insurance Certificates
	CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.14
	Journey Log or Equivalent 
• Presence;
• If the content of Journey logbook/General Declaration or equivalent complies with the requirement;
• For properly filled in; and
• When EFBs are used to display aircraft conditions (e.g. TLB or Journey logbook):
     - Data are up-to-date, and
     - Synchronised correctly according to    operator procedures.
	CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
ORO.MLR.100
ORO.MLR.110
	
	
	
	

	1.15
	Technical Log 
• For any deferred defects (specify in the report where necessary);
• If defects have been properly reported and assessed:
     - Associated maintenance actions have been properly reported, e.g. description of the action, AMM/SRM or other approved data references.
• If open deferred defects remain within time limits, when defect deferments include time limits;
• The compliance of the deferred defects with the aircraft MEL, if available;
• If the rectification intervals stated in the aircraft technical log book (ATLB) do not exceed those required by the MEL (if available).
• When EFBs are used to display aircraft conditions (e.g. TLB or Journey logbook), the data are up-to-date and synchronized correctly according to operator procedures.
• If warning messages (e.g. ECAM/EICAS messages) have been properly reported and assessed.
	CAT.OP.MPA. 175
CAT.IDE.A.105 
CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.16
	Details of the filed ATS flight plan 
(if applicable)
	CAT.OP.MPA. 177
CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.17
	The current parts of the operations manual that are relevant to the duties of the crew.
	CAT.GEN.MPA.100
CAT.GEN.MPA.105
CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.18
	Minimum Equipment List (MEL)
	CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
CAT.IDE.A.105
ORO.MLR.105
	
	
	
	

	1.19
	Appropriate Notices to Airmen (NOTAMs) and Aeronautical Information Service (AIS) briefing documentation
	CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.20
	Appropriate meteorological information
	CAT.GEN.MPA.105
CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.21
	Cargo and/or passenger manifests 
(if applicable)
	CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.22
	Mass and balance documentation/
Calculation Inspect for:
• The presence of a completed mass and balance (M&B) sheet (either paper or digital format).
• M&B sheet calculations: 
     - Are within the a/c limits during any phase of the operation. 
     - Are accurate. 
     - Consider actual load distribution.
     - Pilots acceptance.
	CAT.GEN.MPA.105
CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
CAT.POL.MAB.100(a), CAT.POL.MAB.105(a), CAT.POL.A.
105(a)
ORO.GEN.110  
	
	
	
	

	1.23
	Operational flight plan & Dispatch Release
	CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
CAT.OP.MPA.
175(a)
CAT.OP.MPA.
182
CAT.POL.A.
105(a)(2)
CAT.GEN.MPA.105
	
	
	
	

	1.24
	Notification of special categories of passenger (SCPs) and special loads 
(if applicable)
	CAT.GEN.MPA.180, 
AMC1 CAT.GEN.MPA.180(a) GM1 CAT.GEN.MPA.180(a)(1)
	
	
	
	

	1.25
	Oxygen Equipment 
• Presence;
• Access;
• Condition;
• If the oxygen masks allow for a quick donning (rapid fitment);
• Oxygen cylinder pressure. In case of low pressure, check the minimum required according to the operations manual/flight manual.
	CAT.IDE.A.235 
CAT.IDE.A.240
CAT.IDE.A.100
(e)
CAT.IDE.A.245 CAT.OP.MPA.
285  
	
	
	
	

	1.26
	PBE (Protective Breathing Equipment)
	CAT.IDE.A.245 (b)
AMC1 CAT.IDE.A.245
	
	
	
	

	1.27
	Crash Axe & Crowbar
	CAT.IDE.A.255
	
	
	
	

	1.28
	Independent portable light
• If appropriate portable lights are readily available at all crew member stations.
• The serviceability.
• The accessibility.
	CAT.IDE.A.115
(a)(4)
	
	
	
	

	1.29
	Flight Crew License & Rating / English Language Proficiency
	TCAR Part FCL.045
TCAR Part FCL.055
	
	
	
	

	1.30
	Flight Crew Medical Certificate
	TCAR Part FCL.040
TCAR Part FCL.045
	
	
	
	

	1.31
	Maintenance Release 
Note: Check that the Pilot-in-Command certified that a maintenance release has been issued
	CAT.OP.MPA. 175(b)(1)
	
	
	
	

	1.32
	Defect notification and rectification
	CAT.OP.MPA. 175(b)(1)
CAT.GEN.MPA.100(b)(1)
CAT.GEN.MPA.105(a)(11)
ORO.MLR.105
(e)(3)
ORO.MLR.105
(g)
CAT.GEN.MPA.105 
Technical Log Procedures
	
	
	
	

	1.33
	Pre-Flight Inspection
	CAT.GEN.MPA.105(a)(1)(2)(8)
(11)(12)
CAT.OP.MPA. 175(b)(1)
	
	
	
	

	1.34
	Refueling Procedures
	CAT.OP.MPA.
195

	
	
	
	

	2
	Cabin Interior

	2.1

	General Condition
Inspect:
• The general condition, including lavatories (general condition and smoke detection systems), flammable furnishings;
• The stowage of baggage/equipment, or heavy/hard pointed objects which might be stored in the toilets (waste bags temporarily stowed in a locked toilet is considered acceptable);
• If service carts manufactured after 4 November 2005 for proper braking action;
  - Findings should only be raised in those cases where the braking action is obviously not meeting the standard. Carts with defective brakes may be used as storage carts in the galley as long as such defective carts are properly labelled.
• If markings required by operational or registration Authorities are installed, as well as passenger and crew placards and illuminated signs for safety equipment.
Notes:
       - Special attention when checking cabin items which may result in an unsafe situation (e.g. stowage of a single catering box where pairs are required; weight limitation of catering containers).
       - Where loose and unsecured (passenger) luggage is found in the cabin, this should be reported under “Safety of Cabin Baggage”. Where it concerns loose luggage, which might block the emergency exit, in that case the finding should be under “Access to emergency exits”.
	CAT.IDE.A.205.
ORO.GEN.110
CAT.OP.MPA. 230
CAT.OP.MPA. 160
CS 25.854
ICAO Annex 8  

	
	
	
	

	2.2

	Cabin crew’s station & crew rest area
• General condition and serviceability of the cabin crew seats;
• Presence and condition of the safety harness and/or belt; and
• Accessibility of life jackets.
• The serviceability of the communication system (Cockpit to Cabin and Cabin to Cabin). In case of unserviceability, check against the MEL.
• Cabin crew seats not correctly located
	CAT.IDE.A.205
CS 25.785(h)
	
	
	
	

	2.3

	First Aid Kit/Emergency Medical Kit 
• Presence;
• Accessibility; and
• Identification of medical supplies (first aid kit(s) and, if applicable, emergency medical kit and universal precaution kit).
• Number of first-aid kits required
Notes:
       - Medical supplies without a date does not constitute a finding. However, if stated expiry date has been exceeded, then this should be reported as a finding
	CAT.IDE.A.220 
CAT.IDE.A.225
CAT.GEN.MPA.105(a)(7)
CAT.OP.MPA. 170
CAT.IDE.A.100 (e)
CAT.IDE.A.220
	
	
	
	
	Number of pax 100-200 > Number of first aid kits required 2

	2.4

	Hand fire extinguishers
• If at the indicated location and easily accessible;
• If they are correctly secured in their bracket;
• If they are marked with the appropriate operating instructions;
• If they are serviceable (including the extinguishing agent release mechanism):
    - Check pressure gauge (if installed), check expiration date (if any).
    - If considerably low weight, consider it unserviceable.
• The number of serviceable extinguishers against the minimum number required, taking into consideration the applicable MEL references (if applicable).
	CAT.IDE.A.250
CAT.IDE.A.100 (e)
CAT.OP.MPA. 230
	
	
	
	

	2.5

	Lifejackets/flotation devices 
• Presence;
• Access; and
• Sufficient number and serviceability
	CAT.IDE.A.305
CAT.IDE.A.285 (a)(b)
CAT.IDE.A.100 (e)
	
	
	
	

	2.6

	Seat belt and seat condition
• The condition of seats and belts;
• The condition of under seat baggage restraining bar;
• The availability and condition of extension belts (if needed).
	CAT.IDE.A.205  
AMC1 CAT.IDE.A.205
AMC2 CAT.IDE.A.205 
AMC3 CAT.IDE.A.205 
GM1 CAT.IDE.A.205
GM2 CAT.IDE.A.205
	
	
	
	

	2.7
	Emergency exit, lighting / marking, independent portable light
• Presence and condition of the emergency exit signs, lighting and marking;
• Presence and condition of an escape path illumination system;
• Presence and condition of the visual indication of the path to emergency exits in smoke filled cabins;
• Presence of operating instructions on the emergency exits;
• Appropriate independent portable lights are readily available at all crew member stations and their condition.
	CAT.IDE.A.115 (a)(4)
CAT.GEN.MPA.105(a)(11)
CAT.IDE.A.275 (a)(b)(4)(5) 
CAT.IDE.A.265
	
	
	
	

	2.8
	Access to emergency exits
• Floor/carpets/panels condition;
• Access to emergency exits not impeded by baggage/seats/tables; and
• Provisions about occupancy of seats by over wing exit are in place and complied with
	CAT.OP.MPA. 160           
AMC1 CAT.OP.MPA. 160(f)(g)
CAT.OP.MPA. 165
AMC1 CAT.OP.MPA. 165(a)(b)(c)
CAT.OP.MPA. 230
	
	
	
	

	2.9

	Slide rafts/life rafts (as required) 
and ELT
• For number and serviceability of slides/slide rafts/life rafts.
• The presence and type of ELT(s) and serviceability.
• If required ELT(s) transmit on 406 MHz and 121.5 MHz frequencies.
• The equipment for pyrotechnical distress signals (if required and easily accessible).
	CAT.IDE.A.305
CAT.IDE.A.280  
CAT.IDE.A.285 (d)(e)
	
	
	
	

	2.10

	Oxygen supply (cabin crew and passengers)
• The cabin oxygen quantity (pressure gauge or electronic display) when stored oxygen is used;
• The number / serviceability of oxygen dispensing units or oxygen masks (if applicable and possible); and
• If oxygen equipment (bottles and masks) is stowed at the indicated location.
	CAT.IDE.A.230
CAT.IDE.A.240
CAT.IDE.A.285 
CAT.IDE.A.235 (a)(b)(c)(d)(e)  
	
	
	
	

	2.11
	Protective breathing equipment (PBE)
• Availability;
• Stored at the indicated location;
• Adequately marked with its operating instructions;
• Serviceability;
• In minimum required number (against MEL, when applicable).
	CAT.IDE.A.245
	
	
	
	

	2.12
	Safety instructions
• The accuracy of the passenger emergency briefing cards and sufficient available numbers, or any alternative method to convey the required information;
• The information given to the passengers concerning: location of life vest, oxygen equipment, access doors;
• Serviceability of the “Fasten seat belt” and “Return to seat” (lavatories) signs, if installed (when unserviceable check against MEL provisions if applicable).
	CAT.GEN.MPA.105(a)(7)
CAT.OP.MPA. 170
CAT.IDE.A.210
	
	
	
	

	2.13
	Cabin crew members 
• Cabin crew composition meets the minimum crew requirements (available in the operations manual).
• Cabin crew members are familiar with the cabin emergency procedures and the location and/or operation of the emergency equipment.
• Cabin crew members are in compliance with the flight and duty time rules contained within the operations manual when circumstances dictate (e.g. aircraft undergoes significant delay).
	CAT.GEN.MPA.100(b)(4)
ORO.MLR.100 (a)(b)
ORO.CC.100
	
	
	
	

	2.14
	Stowage of passenger’s baggage
• Stowage of baggage (including heavy and oversized baggage);
• Condition of the overhead bins.
	CAT.OP.MPA. 160 
AMC1 CAT.OP.MPA. 160
AMC2 CAT.OP.MPA. 160



	
	
	
	

	3
	Aircraft Exterior

	3.1 


	General Condition 
• Corrosion;
• Legibility of markings;
• Loose or missing fasteners and rivets;
• Missing or damaged bonding wires;
• Presence and condition of the antennas;
• Presence and condition of the static dischargers;
• Condition and functionality of the exterior lighting;
• Condition of the pressure ports (static ports and pitot tubes) and the RVSM areas (if any);
• Break-in point markings (if applied) faded or incorrectly marked.
	CAT.IDE.A.260
CAT.IDE.A.275 (a)(b)(4)(5)
TCAR 8, Part M
	
	
	
	

	3.2

	Doors and hatches
• Condition of doors, hatches and associated seals;
• Presence and condition of bonding wires;
• Loose or missing fasteners and rivets; and
• Door external markings, operation instructions.
	
	
	
	
	

	3.3

	Flight Controls 
• The external flight controls;
• For hydraulic leakage;
• For presence and condition of the static dischargers;
• For presence and condition of bonding wires; and
• For loose or missing fasteners and rivets.	
	CAT.OP.MPA. 175(b)(1)
	
	
	
	

	3.4
	Wheels, tyres and brakes
• The wheels and tyres for damage and wear;
• When possible, for correct tyre pressure;
• Brake system; and
• The landing gear snubbers.	
	
	
	
	
	

	3.5 
	Undercarriage, skids / floats 
• The condition, lubrication, corrosion, leaks, damage and inappropriate strut extension;
• For presence and legibility of inspection markings/placards;
• The skids/floats for obvious damages; and
• For presence and condition of the water/debris deflectors (if required to be installed).

	
	
	
	
	

	3.6
	Wheel Well 
• Damage;
• Lubrication, leakage & corrosion and wear on door fittings and hinges;
• Loose or missing fasteners and rivets; and
• Presence and condition of bonding wires.
	
	
	
	
	

	3.7
	Power plant and Pylon 
• Dents;
• Loose/missing fasteners and rivets;
• Obvious damage to sensors;
• Cracks;
• Panels if they are aligned and handles are flush;
• Unusual damage and leaks;
• Condition of the thrust reverser;
• Condition of the Intake acoustic liners; and
• Presence and legibility of the markings and placards.
	
	
	
	
	

	3.8
	Fan blades, propellers, rotors (main & tail)
• For FOD damage, cracks, cuts, corrosion, erosion, etc;
• The LPT/LPC blades and IGV/OGV (where visible);
• For corrosion, looseness of blades in hub, stone damage, etc; and
• The de-icing boots for damage (where fitted).
	
	
	
	
	

	3.9
	Obvious Repairs 
• Repairs of unusual design or poorly performed.
	
	
	
	
	

	3.10
	Leakage 
• Fuel leaks;
• Hydraulic leaks; and
• Toilet liquid leaks (blue ice, if applicable)	
	
	
	
	
	

	4
	Cargo & Loading

	4.1
	General condition  
• The general condition of cargo compartment;
• The lighting, fire protection, detection & extinguishing system (if appropriate);
• The side wall and overhead (blow-out) panels, smoke detectors, smoke barrier/curtain; and
• For the presence and condition of cargo barrier/dividing nets.
	
	
	
	
	

	4.2
	Dangerous Goods (if applicable)
	Annex 18, ICAO Document 9284 (Technical Instructions)
	
	
	
	

	4.3
	Secure stowage of cargo on board
• That loads are properly distributed (floor limits, height limits, pallets and containers maximum gross weight);
• That flight/fly-away kit and spare wheels are correctly secured;
• That cargo is correctly secured;
• The condition of cargo containers, pallets, lock assemblies and lashing nets; and
• The condition of the cargo compartment dividing nets.
	CAT.OP.MPA. 160
CAT.OP.MPA. 175(b)(1)
	
	
	
	



S = Satisfied
U= Unsatisfied   
N/A= Not Applicable
Comment= Description the detail of compliance or Non Compliance or other information

		Inspector Name:………………………………………………………………….………
		                      (………………………………….………..……………………….….)
		Position:…………………………………………….…………………………………………
Completed on:…………………………………………………………………………….
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