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Checklist Number:                   OPS-TCGEN-307                                                             
Checklist Name:  OPS-AIR-ADS-B-Automatic Dependent Surveillance–Broadcast
Applicability:                                                                                                                                        
Location:                                                                      Date:                                       



	
	
	



	No
	Subject
	Reference
	S
	U
	N/A
	Comment

	0
	Preliminary (OPS and AW)
	
	
	
	
	

	0.1
	Operator (For AOC):

	
	
	
	
	

	0.2
	Aircraft Registration/s (Non AOC):

	
	
	
	
	

	0.3
	Aircraft Make and Model:

	
	
	
	
	

	0.4
	Initial Approval (Yes/No)

	
	
	
	
	

	0.5
	Additional Aircraft (Yes/No)

	
	
	
	
	

	0.6
	List of aircraft (registration No. and Serial No.) requested for ADS-B approval

	
	
	
	
	

	0.7
	Inspectors Name (Airworthiness)

	
	
	
	
	

	0.8
	Inspectors Name (Flight Operations)

	
	
	
	
	

	0.9
	Date of Review

	
	
	
	
	

	1
	ADS-B Status (AW)
	
	
	
	
	

	1.1
	Check the AFM and TCDS and confirm the Aircraft’s ADS-B Status? May be a manufacturers letter. 

The Aircraft Flight Manual (AFM) or the Pilot’s Operating Handbook (POH), whichever is applicable, needs to provide at least a statement of compliance that the ADS-B System complies with EASA AMC20-24 and if deviations are applicable. Deviations, including those stated in EASA AMC 20-24, as appropriate may be included or referred to.


	GM for FANS item 1.3, 2.5.4

	
	
	
	

	1.2
	Confirm the ADS-B installation complies with EASA CS-ACNS, AMC20-24 or an other standard acceptable to CAAT
	GM for FANS item 2.2
	
	
	
	

	1.3
	Are there limitations and abnormal procedures in the AFM relating to ADS-B?
	GM for FANS item 2.4.1, 2.4.2, 2.5.4 (c)
	
	
	
	

	1.4
	Has a unique ICAO 24 bit aircraft address been assigned by CAAT to each airframe.
	
	GM for FANS item 2.5.4 (d)
	
	
	
	

	2
	Maintenance Programme and MEL (AW)
	
	
	
	
	

	2.1
	Does the AMP contain tasks related to ADS-B?
	GM for FANS item 2.5.4 (e)
	
	
	
	

	2.1.1
	Do the Maintenance tests include a periodic verification check of aircraft derived data including the ICAO 24 bit aircraft address using suitable ramp test equipment. The check of the 24 bit aircraft address should be made also in the event of a change of state of registration of the aircraft.
	GM for FANS item 2.5.4 (d)
	
	
	
	

	2.1.2
	Do the maintenance tests include checks to check the correct functioning of system fault detectors
	GM for FANS item 2.5.4 (d)
	
	
	
	

	2.1.3
	Do the maintenance tests include ADS-B transmit system level tests for encoding altitude sensors with Gillham’s code output (should be based on the transition points defined in EUROCAE ED-26, Table 13).
	GM for FANS item 2.5.4 (d)
	
	
	
	

	2.1.4
	Has the periodicity for the check of the ADS-B transmitter been established.
	GM for FANS item 2.5.4 (e) 
	
	
	
	

	2.2
	Does the AMO/MRO have access to the required manuals (e.g. MM, CMM) referenced in the AMP?
	GM for FANS item 2.5.4 (d), 2.8.1 (e) (i)

	
	
	
	

	2.3
	Does the MEL address the required equipment for ADS-B operations?
	GM for FANS item 2.5.4 (f), 2.8.1 (e) (ii)
	
	
	
	

	3
	Operators Maintenance Arrangements (AW)
	
	
	
	
	

	3.1
	Does the Operator’s GMM reflect ADS-B arrangements to the associated or contracted AMO/MRO. 

Note: May be covered under general maintenance arrangements
	GM for FANS item 2.8.1 (e) (i)
	
	
	
	

	3.2
	If maintenance is contracted to an outside AMO/MRO does the contract reflect ADS-B?

Note: May be covered under general maintenance
	
	
	
	
	

	3.3
	Does the GMM contain occurrence reporting arrangements?
	GM for FANS item 2.5.4 (i)
	
	
	
	

	3.4
	Does the AMO/MRO have the appropriate tooling and test equipment
	GM for FANS item 2.5.4 (d) 
	
	
	
	

	4
	Personnel and Training (AW)
	
	
	
	
	

	4.1
	Are the operators and AMO/MRO maintenance personnel trained for ADS-B?
	GM for FANS item 1.3.4
	
	
	
	

	5
	Operations Manual (OPS)
	
	
	
	
	

	5.1
	Does the Operations Manual include a system description, operational and contingency procedures and training elements for use of the ADS-B-NRA application. 

Note: The Operations Manual, preferably OM-B, should contain the operational aspects described in EASA AMC 20-24.
	ORO.MLR.101
GM for FANS item 2.5.4

	
	
	
	

	5.2
	Does the Ops Manual include the requirements of flight crew actions/intervention
	ORO.MLR.101
GM for FANS item 2.4.1
	
	
	
	

	5.3
	Does the Ops manual contain procedures for training—The operator must provide training to each flight crew member involved with ADS-B operations.
	ORO.MLR.101
GM for FANS item 2.5.4 (g)

	
	
	
	

	6
	Flight Crew Training (OPS)
	
	
	
	
	

	6.1
	Is there ADS-B training in place?   (Note where the training is defined)
	GM for FANS item 2.5.4 (g)
	
	
	
	

	6.2
	Does the training address general understanding of ADS-B-NRA operating procedures;
	GM for FANS item 2.5.4 (g)
	
	
	
	

	6.3
	Does the training address specific ADS-B associated phraseology;
	GM for FANS item 2.5.4 (g) (ii)
	
	
	
	

	6.4
	Does the training address general understanding of the ADS-B technique and technology;
	GM for FANS item 2.5.4 (g) (iii)
	
	
	
	

	6.5
	Does the training address characteristics and limitations of the flight deck human-machine interface, including an overview of ADS-B environment and system descriptions;
	GM for FANS item 2.5.4 (g) (v) 
	
	
	
	

	6.6
	Does the training address the need to use the ICAO defined format for entry of the Aircraft Identification or Aircraft Registration marking as applicable to the flight;
	GM for FANS item 2.5.4 (g) (vi) 
	
	
	
	

	6.7
	Does the training address operational procedures regarding the transmission of solely the generic emergency flag in cases when the flight crew actually selected a discrete emergency code (if implemented, refer to section 8.8 of EASA AMC 20-24 ) and SPI;
	GM for FANS item 2.5.4 (g) (vii) 
	
	
	
	

	6.8
	Indication of ADS-B transmit capability within the ICAO flight plan but only when the aircraft is certified according to this AMC;
	GM for FANS item 2.5.4 (g) (viii) 
	
	
	
	

	6.9
	Does the training address handling of data source errors (e.g. discrepancies between navigation data sources)? 

(If flight crew receive equipment indications showing that position being broadcast by the ADS-B system is in error (e.g. GPS anomaly), they should inform the ATSP, as appropriate, using any published contingency procedures.)
	GM for FANS item 2.5.4 (g) (ix)
	
	
	
	

	6.10
	Does the training address Incident reporting procedures
	GM for FANS item 2.5.4 (g) (xi) 
	
	
	
	

	6.11
	Does the training address Crew Resources Management and associated human factors issues.
	GM for FANS item 2.5.4 (g) (xii) 
	
	
	
	

	7
	Incident Reporting Procedures (OPS and AW)
	
	
	
	
	

	7.1
	Does the operator have procedures in place for reporting significant incidents associated with ATC surveillance information transmitted by the ADS-B data link that affects or could affect the safe operation of the aircraft.   (Record where these are provided)
	GM for FANS item 2.5.4 (i)
	
	
	
	






S = Satisfied
U= Unsatisfied   
N/A= Not Applicable
Comment= Description the detail of compliance or Non Compliance or other information

		Inspector Name: ………………………………………………………………….………
		                      (………………………………….………..……………………….….)
		Position: …………………………………………….…………………………………………
Completed on: …………………………………………………………………………….
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