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	FLIGHT SIMULATOR EVALUATION AND CERTIFICATION CHECKLIST/REPORT


	General Information

	NAME OF FSTD ORGANISATION

	TYPE / VARIANT OF AIRCRAFT

	TYPE OF FSTD


	SIMULATOR LOCATION

	SERIAL NUMBER

	TYPE OF EVALUATION


	INSPECTOR NAME

	DATE OF EVALUATION

	FSTD Certificate Number




	PRE-EVALUATION DOCUMENT REVIEW



	1. Document Verification (Initial)

	Ref
	Document / Requirement
	Regulatory Reference
	Result

	DOC-I1
	Certificate or official document confirming legal status, objectives, registered address, and authorized signatories.
	R2CAAT No. 77 Clause 38 (1)
	

	Comment
	

	DOC-I2
	Document evidencing ownership or lawful possession of the FSTD.
	R2CAAT No. 77 Clause 38 (2)
	

	Comment
	

	DOC-I3
	Organisation chart and responsible persons for supervision and maintenance.
	R2CAAT No. 77 Clause 38 (3)
	

	Comment
	

	DOC-I4
	Layout of the flight training device installation site.
	R2CAAT No. 77 Clause 38 (4)
	

	Comment
	

	DOC-I5
	Master Qualification Test Guide (MQTG) (if any).
	R2CAAT No. 77 Clause 38 (5)
	

	Comment
	

	DOC-I6
	Qualification Test Guide (QTG).
	R2CAAT No. 77 Clause 38 (6)
	

	Comment
	

	DOC-I7
	User guide manual for the FSTD.
	R2CAAT No. 77 Clause 38 (7)
	

	Comment
	

	DOC-I8
	Other documents or evidence as specified by the competent authority.
	R2CAAT No. 77 Clause 38 (8)
	

	Comment
	



	2. Document Verification (Renewal)

	Ref
	Document / Requirement
	Regulatory Reference
	Result

	DOC-R1
	Copy of Current/Previous CAAT FSTD Certificate.
	R2CAAT No. 77 Clause 42 (1)
	

	Comment
	

	DOC-R2
	Any changed documents (No.1 to No.8) since initial certification.
	R2CAAT No. 77 Clause 42 (2)
	

	Comment
	

	DOC-R3
	Record of Daily function pre-flight check.
	R2CAAT No. 77 Clause 42 (3)
	

	Comment
	

	DOC-R4
	Record of Daily discrepancy log and corrections.
	R2CAAT No. 77 Clause 42 (4)
	

	Comment
	



	3. Document Review (Pre-Evaluation)

	Ref
	Document / Requirement
	Regulatory Reference
	Result

	FAQ-F1
	Does the current Configuration Management record for this FSTD accurately identify: host computer hardware and software version; visual system version; motion system status; IOS software version; and 
	ORA.FSTD.110
	

	Comment
	

	FAQ-F2
	Where modifications affecting the QTG have been incorporated since the last evaluation — is there documented evidence that the affected validation tests were amended before the FSTD returned to servic
	ORA.FSTD.110
	

	Comment
	

	FAQ-F3
	Does the technical log for this FSTD record all defects, deferred defects, and development work with: date raised; description; action taken; responsible person; and date closed?
	ORA.FSTD.240
	

	Comment
	

	FAQ-F4
	Is the current deferral register for this FSTD available and up to date? Are deferred defects reviewed at defined intervals with sign-off confirming they do not affect safety or adequacy of training?
	ORA.GEN.200(a)(1)(v)
	

	Comment
	

	FAQ-F5
	Are navigational database update records for this FSTD maintained, showing: current AIRAC cycle installed; date of last update; and responsible person?
	ORA.FSTD.110, .240
	

	Comment
	

	FAQ-F6
	Is the navigational database version currently installed in this FSTD consistent with the version declared in the evaluation dossier?
	ORA.FSTD.110
	

	Comment
	

	FAQ-F7
	Is the FSTD qualification certificate for this device currently valid (not expired) and immediately accessible at the FSTD facility?
	ORA.FSTD.225
	

	Comment
	

	FAQ-F8
	Does the qualification certificate specify all required fields: FSTD type and level; aircraft/class simulated; approved configurations; functionalities; and any restrictions or limitations?
	ORA.FSTD.225
	

	Comment
	

	FAQ-F9
	Is the most recent annual FSTD safety feature check record for this device available, signed off by the responsible person, and dated within the preceding 12 months?
	ORA.FSTD.115
	

	Comment
	

	FAQ-F10
	Is there evidence that safety briefings have been delivered to current FSTD occupants and maintenance personnel for this device?
	ORA.FSTD.115
	

	Comment
	

	FAQ-F11
	Does the modification log for this FSTD record all hardware and software changes since initial qualification, including date, description, classification (major/minor), and approval status?
	ORA.FSTD.110
	

	Comment
	

	FAQ-F12
	For any major modifications to this FSTD — has CAAT been notified in advance and has CAAT's determination on whether a special evaluation was required been obtained and documented?
	ORA.FSTD.110, GM1
	

	Comment
	

	FAQ-F13
	Where this FSTD has been relocated since initial qualification — was CAAT notified before the move; were at least one-third of validation tests and function/subjective tests completed before return to
	ORA.FSTD.230
	

	Comment
	

	FAQ-F14
	Where this FSTD has been deactivated for a prolonged period — was CAAT notified; was a reactivation plan agreed; and were reactivation tests completed and documented before return to service?
	ORA.FSTD.230
	

	Comment
	

	FAQ-F15
	Where there has been a transfer of qualification for this FSTD to a new operating organisation — was CAAT informed in advance; was a transfer plan agreed; and is the certificate valid under the new op
	ORA.FSTD.235
	

	Comment
	



	4. FSTD Walkaround

	Ref
	Document / Requirement
	Regulatory Reference
	Result

	FAQ-W1
	Motion system area — external markings and access control
	AMC1 ORA.FSTD.115
	

	Comment
	

	FAQ-W2
	External motion system warning indicators
	AMC1 ORA.FSTD.115
	

	Comment
	

	FAQ-W3
	Guard rails, gates, and stairway access
	AMC1 ORA.FSTD.115
	

	Comment
	

	FAQ-W4
	Fire extinguishers and suppression equipment — external
	AMC1 ORA.FSTD.115
	

	Comment
	

	FAQ-W5
	Qualification certificate posted or accessible at or near entry
	ORA.FSTD.225
	

	Comment
	

	FAQ-W6
	Safety briefing notices posted
	ORA.FSTD.115
	

	Comment
	

	FAQ-W7
	Emergency stop controls — pilot seats
	AMC1 ORA.FSTD.115
	

	Comment
	

	FAQ-W8
	Emergency stop control — IOS position
	AMC1 ORA.FSTD.115
	

	Comment
	

	FAQ-W9
	Two-way communication system — cockpit to IOS
	AMC1 ORA.FSTD.115
	

	Comment
	

	FAQ-W10
	Escape exits — cockpit/cab
	AMC1 ORA.FSTD.115
	

	Comment
	

	FAQ-W11
	Emergency lighting — cockpit/cab
	AMC1 ORA.FSTD.115
	

	Comment
	

	FAQ-W12
	Fire/smoke detection — inside FSTD cab
	AMC1 ORA.FSTD.115
	

	Comment
	

	FAQ-W13
	IOS — daily function check log
	GM2 ORA.FSTD.100
	

	Comment
	

	FAQ-W14
	IOS — navigational database version displayed
	ORA.FSTD.110
	

	Comment
	

	FAQ-W15
	IOS — configuration build/software version displayed
	ORA.FSTD.110
	

	Comment
	

	FAQ-W16
	Defect logbook / tracking system — current entries
	ORA.FSTD.240
	

	Comment
	

	FAQ-W17
	Additional equipment — not part of original qualification
	ORA.FSTD.120
	

	Comment
	

	FAQ-W18
	Emergency lighting — facility
	AMC1 ORA.FSTD.115
	

	Comment
	

	FAQ-W19
	Escape routes — facility
	AMC1 ORA.FSTD.115
	

	Comment
	

	FAQ-W20
	Fire/smoke detection and suppression — facility
	AMC1 ORA.FSTD.115
	

	Comment
	

	FAQ-W21
	Electrical safety and plant room access
	AMC1 ORA.FSTD.115
	

	Comment
	

	FAQ-W22
	General housekeeping and safety
	ORA.FSTD.115
	

	Comment
	

	FAQ-W23
	Visual system projectors and domes (if applicable)
	ORA.FSTD.225
	

	Comment
	

	FAQ-W24
	Motion system — general condition
	ORA.FSTD.225
	

	Comment
	



	5. QTG, MQTG and FSTD Qualification

	Ref
	Document / Requirement
	Regulatory Reference
	Result

	FAQ-Q1
	Does the MQTG exist, is it the current master version, and does it carry an issue number, effective date, and document control status?
	ORA.FSTD.105
	

	Comment
	

	FAQ-Q2
	Does the MQTG identify the CS-FSTD(A/H) version (issue and effective date) that constitutes the qualification basis?
	ORA.FSTD.210(1)
	

	Comment
	

	FAQ-Q3
	Is the aircraft reference data source documented — manufacturer flight test report, AFM/POH, or engineering data package? For FNPT: is class-level performance data used as the reference?
	ORA.FSTD.210(2)
	

	Comment
	

	FAQ-Q4
	For each test case in the MQTG: does the test ID correspond to a numbered item in the applicable CS-FSTD(A/H) AMC validation test table? Are all mandatory test areas represented (performance, handling
	ORA.FSTD.205, CS-FSTD(A)
	

	Comment
	

	FAQ-Q5
	For each completed test case: is the FSTD output trace plotted against the reference aircraft data? Does the trace remain within the prescribed tolerance band for the complete duration of the manoeuvr
	ORA.FSTD.210
	

	Comment
	

	FAQ-Q6
	Are all MQTG test results dated, marked as analysed and evaluated, and retained per ORA.FSTD.240?
	ORA.FSTD.105, .240
	

	Comment
	

	FAQ-Q7
	Does the QTG status list and recurrent run records confirm that the complete MQTG test set has been run progressively within the preceding 12-month period, as required by ORA.FSTD.105?
	ORA.FSTD.105
	

	Comment
	

	FAQ-Q8
	Where footprint tests are used: is a clear rationale documented in the QTG for each footprint test explaining why manufacturer data was unavailable?
	GM1 ORA.FSTD.200(3)
	

	Comment
	

	FAQ-Q9
	Are footprint test rationales recorded in the Validation Data Roadmap (VDR) per Appendix 2 to AMC1 CS-FSTD(A).300?
	GM1 ORA.FSTD.200(3)
	

	Comment
	

	FAQ-Q10
	Was each footprint test flown by a pilot with current experience on the type, acceptable to CAAT? Does the same pilot sign off the complete test as fully representative?
	GM1 ORA.FSTD.200(2)(iv)
	

	Comment
	

	FAQ-Q11
	Is the original Initial Evaluation Package (dossier) available and retained, including all seven elements required by GM3 ORA.FSTD.100 items (1) through (7)?
	ORA.FSTD.240, AMC1
	

	Comment
	

	FAQ-Q13
	Is the initial CAAT evaluation report available and retained for the lifetime of the device?
	AMC1 ORA.FSTD.240(1)(iv)
	

	Comment
	

	FAQ-Q14
	Is the FSTD qualification certificate from initial evaluation available and retained for the lifetime of the device?
	AMC1 ORA.FSTD.240(1)(iii)
	

	Comment
	

	FAQ-Q12
	Does the organisation have an internal process that assigns a named responsible person to review regular QTG reruns and conduct function/subjective tests?
	ORA.FSTD.225(b)(4)
	

	Comment
	

	FAQ-Q13
	Where extended validity (up to 36 months) has been granted under ORA.FSTD.225(b): has the assigned person reviewed QTG reruns and function/subjective tests within the preceding 12 months and submitted
	ORA.FSTD.225(b)(4)
	

	Comment
	



	FLIGHT SIMULATION TRAINING DEVICE STANDARDS

	
	FLIGHT SIMULATION TRAINING DEVICE STANDARDS
	FFS LEVEL
	FTD
	FNPT LEVEL
	BITD
	REMARKS

	
	
	A
	B
	C
	D
	1
	2
	I
	II
	MCC
	
	

	1. General

	1.a.1
	A fully enclosed flight deck.
	
	
	
	
	
	
	
	
	
	
	

	1.a.2
	Cockpit sufficiently enclosed to exclude distraction, replicating the aeroplane/class.
	
	
	
	
	
	
	
	
	
	
	

	1.a.3
	Flight deck, a full-scale replica of the aeroplane simulated.
	
	
	
	
	
	
	
	
	
	
	

	1.a.4
	Direction of movement of controls and switches identical to the aeroplane.
	
	
	
	
	
	
	
	
	
	
	

	1.a.5
	Full-size panel of replicated system(s) with controls replicating the aeroplane.
	
	
	
	
	
	
	
	
	
	
	

	1.a.6
	Cockpit switches, instruments, panels, controls sufficient for training, spatially correct.
	
	
	
	
	
	
	
	
	
	
	

	1.a.7
	Crew seats with sufficient adjustment for design eye reference position.
	
	
	
	
	
	
	
	
	
	
	

	1.b.1
	Circuit breakers that affect procedures and/or result in observable cockpit indications properly located and functionally accurate.
	
	
	
	
	
	
	
	
	
	
	

	1.c.1
	Flight dynamics model for drag, thrust, attitude, sideslip, altitude, temp, weight, CG, config.
	
	
	
	
	
	
	
	
	
	
	

	1.d.1
	All instrument indications respond to control movement or induced disturbance.
	
	
	
	
	
	
	
	
	
	
	

	1.d.2
	Lighting environment for panels and instruments sufficient for the operation.
	
	
	
	
	
	
	
	
	
	
	

	1.d.3
	Instrument indications respond to icing effects.
	
	
	
	
	
	
	
	
	
	
	

	1.e.1
	Comms, nav, caution/warning equipment corresponding to the aeroplane.
	
	
	
	
	
	
	
	
	
	
	

	1.e.2
	Nav equipment for the aeroplane/class, including comms.
	
	
	
	
	
	
	
	
	
	
	

	1.e.3
	Nav data with approach facilities; aids usable within range.
	
	
	
	
	
	
	
	
	
	
	

	1.f.1
	Three seats for instructor, examiner and authority inspector.
	
	
	
	
	
	
	
	
	
	
	

	1.g.1
	Systems simulate aeroplane operation for normal, abnormal, emergency procedures.
	
	
	
	
	
	
	
	
	
	
	

	1.g.2
	Stick pusher - forces, displacement, surface position correspond to aeroplane.
	
	
	
	
	
	
	
	
	
	
	

	1.h.1
	Instructor controls for system variables and abnormal/emergency conditions.
	
	
	
	
	
	
	
	
	
	
	

	1.h.2
	Real-time feedback tool for training envelope / limit exceedance.
	
	
	
	
	
	
	
	
	
	
	

	1.h.3
	Upset scenarios: IOS selectable upsets with guidance.
	
	
	
	
	
	
	
	
	
	
	

	1.i.1
	Control forces and travel correspond to the aeroplane.
	
	
	
	
	
	
	
	
	
	
	

	1.j.1
	Ground handling/aerodynamics: ground effect, reaction, handling.
	
	
	
	
	
	
	
	
	
	
	

	1.k.1
	Wind shear models for recognition/recovery in critical phases.
	
	
	
	
	
	
	
	
	
	
	

	1.l.1
	Instructor controls for environmental effects (wind speed/direction).
	
	
	
	
	
	
	
	
	
	
	

	1.m.1
	Stopping/directional control for dry, wet, icy, patchy, rubber residue.
	
	
	
	
	
	
	
	
	
	
	

	1.n.1
	Brake/tyre failure dynamics (antiskid) and brake temperature effects.
	
	
	
	
	
	
	
	
	
	
	

	1.o.1
	Means for daily testing of FSTD programming and hardware.
	
	
	
	
	
	
	
	
	
	
	

	1.p.1
	Computer capacity, accuracy, resolution, dynamic response sufficient.
	
	
	
	
	
	
	
	
	
	
	

	1.q.1
	Control feel dynamics replicate aeroplane; free response matches.
	
	
	
	
	
	
	
	
	
	
	

	1.r.1
	Transport delay/Latency within 150 ms (300 ms for A/B, FTDs, FNPTs, BITDs).
	
	
	
	
	
	
	
	
	
	
	

	1.s.1
	Aerodynamic modelling: ground effect, Mach, thrust on controls, aeroelastic.
	
	
	
	
	
	
	
	
	
	
	

	1.s.2
	Aerodynamic model covering AoA and sideslip range for training.
	
	
	
	
	
	
	
	
	
	
	

	1.s.3
	Aerodynamic modelling for stall-recovery training.
	
	
	
	
	
	
	
	
	
	
	

	1.t.1
	Icing effects on airframe, aerodynamics, engines (FFS C/D).
	
	
	
	
	
	
	
	
	
	
	

	1.t.2
	Icing effects on airframe, aerodynamics, engines (FNPT-II/MCC).
	
	
	
	
	
	
	
	
	
	
	

	1.u.1
	Aerodynamic/ground reaction modelling for reverse thrust directional control.
	
	
	
	
	
	
	
	
	
	
	

	1.v.1
	Realistic aeroplane mass properties as function of payload and fuel.
	
	
	
	
	
	
	
	
	
	
	

	1.w.1
	Self-testing for FSTD hardware and programming compliance.
	
	
	
	
	
	
	
	
	
	
	

	1.x.1
	Timely update subsequent to aeroplane modification.
	
	
	
	
	
	
	
	
	
	
	

	1.y.1
	Daily preflight documentation.
	
	
	
	
	
	
	
	
	
	
	



	2. Motion System

	2.a.1
	Motion cues representative of the aeroplane.
	
	
	
	
	
	
	
	
	
	
	

	2.b.1
	Motion system: sufficient cueing, min 3 DOF, 6-DOF equivalent.
	
	
	
	
	
	
	
	
	
	
	

	2.c.1
	A means of recording the motion response time.
	
	
	
	
	
	
	
	
	
	
	

	2.d.1
	Motion effects: rumble, buffets, gear, stall, touchdown, etc. (13 items).
	
	
	
	
	
	
	
	
	
	
	

	2.e.1
	Motion vibrations: characteristic modes measurable vs aeroplane data.
	
	
	
	
	
	
	
	
	
	
	

	3. Visual System

	3.a.1
	Visual system meets all applicable standards.
	
	
	
	
	
	
	
	
	
	
	

	3.b.1
	Min collimated FOV: 45 H x 30 V each pilot.
	
	
	
	
	
	
	
	
	
	
	

	3.b.2
	Cross-cockpit FOV: 180 H x 40 V.
	
	
	
	
	
	
	
	
	
	
	

	3.b.3
	Visual (night/dusk/day) min 45 H x 30 V with adjustable cloud/visibility.
	
	
	
	
	
	
	
	
	
	
	

	3.c.1
	A means of recording the visual response time.
	
	
	
	
	
	
	
	
	
	
	

	3.d.1
	System geometry free from optical discontinuities and artefacts.
	
	
	
	
	
	
	
	
	
	
	

	3.e.1
	Visual textural cues for sink rate and depth perception.
	
	
	
	
	
	
	
	
	
	
	

	3.f.1
	Horizon/attitude correlate to attitude indicator.
	
	
	
	
	
	
	
	
	
	
	

	3.g.1
	Occulting - a minimum of ten levels shall be available.
	
	
	
	
	
	
	
	
	
	
	

	3.h.1
	Surface (Vernier) resolution not greater than 2 arc minutes.
	
	
	
	
	
	
	
	
	
	
	

	3.i.1
	Surface contrast ratio not less than 5:1.
	
	
	
	
	
	
	
	
	
	
	

	3.j.1
	Highlight brightness not less than 20 cd/m2 (6ft-lamberts).
	
	
	
	
	
	
	
	
	
	
	

	3.k.1
	Light point size not greater than 5 arc minutes.
	
	
	
	
	
	
	
	
	
	
	

	3.l.1
	Light point contrast ratio not less than 10:1.
	
	
	
	
	
	
	
	
	
	
	

	3.l.2
	Light point contrast ratio not less than 25:1.
	
	
	
	
	
	
	
	
	
	
	

	3.m.1
	Daylight, twilight, night visual capability.
	
	
	
	
	
	
	
	
	
	
	

	3.m.2
	Visual system brightness and contrast ratio criteria.
	
	
	
	
	
	
	
	
	
	
	

	3.m.3
	Total scene content: 10,000 textured surfaces, 6,000/15,000 lights, 16 moving objects.
	
	
	
	
	
	
	
	
	
	
	

	3.m.4
	Daylight: full colour with textural cues for visual approach, landing and taxi.
	
	
	
	
	
	
	
	
	
	
	

	3.m.5
	Twilight: reduced ambient, self-illuminated objects, definable horizon.
	
	
	
	
	
	
	
	
	
	
	

	3.m.6
	Night: all twilight features minus non-self-illuminating ground cues.
	
	
	
	
	
	
	
	
	
	
	

	4. Sound System

	4.a.1
	Significant flight deck sounds for the aeroplane/class.
	
	
	
	
	
	
	
	
	
	
	

	4.b.1
	Precipitation, rain removal, crash sound, significant noises.
	
	
	
	
	
	
	
	
	
	
	

	4.c.1
	Comparable amplitude/frequency of noises coordinated with weather.
	
	
	
	
	
	
	
	
	
	
	

	4.d.1
	Volume control with indication meeting qualification.
	
	
	
	
	
	
	
	
	
	
	





	TABLE OF FUNCTIONS AND SUBJECTIVE TESTS

	
	TABLE OF FUNCTIONS AND SUBJECTIVE TESTS
	FFS LEVEL
	FTD
	FNPT LEVEL
	BITD
	REMARKS

	
	
	A
	B
	C
	D
	1
	2
	I
	II
	MCC
	
	

	1. Preparation for Flight

	1.1A
	Flight deck design/functions identical to the aeroplane or class.
	
	
	
	
	
	
	
	
	
	
	

	1.1B
	Design/functions represent the simulated class of aeroplane.
	
	
	
	
	
	
	
	
	
	
	



	2. Surface Ops (Pre-Take-Off)

	2.1A
	Normal engine start.
	
	
	
	
	
	
	
	
	
	
	

	2.1B
	Alternate start procedures.
	
	
	
	
	
	
	
	
	
	
	

	2.1C
	Abnormal starts and shutdowns (hot, hung, tail pipe fire).
	
	
	
	
	
	
	
	
	
	
	

	2.1D
	Pushback / Powerback.
	
	
	
	
	
	
	
	
	
	
	

	2.2A
	Taxi - Thrust response.
	
	
	
	
	
	
	
	
	
	
	

	2.2B
	Taxi - Power lever friction.
	
	
	
	
	
	
	
	
	
	
	

	2.2C
	Taxi - Ground handling.
	
	
	
	
	
	
	
	
	
	
	

	2.2D
	Taxi - Nosewheel scuffing.
	
	
	
	
	
	
	
	
	
	
	

	2.2E
	Taxi - Brake operation (normal/alternate/emergency).
	
	
	
	
	
	
	
	
	
	
	

	2.2E(a)
	Taxi - Brake fade (if applicable).
	
	
	
	
	
	
	
	
	
	
	

	2.2E(b)
	Taxi - Brake other.
	
	
	
	
	
	
	
	
	
	
	

	3. Take-Off

	3.1A
	Normal - Aeroplane/engine parameter relationships.
	
	
	
	
	
	
	
	
	
	
	

	3.1B
	Normal - Acceleration characteristics (motion).
	
	
	
	
	
	
	
	
	
	
	

	3.1C
	Normal - Acceleration characteristics (non-motion).
	
	
	
	
	
	
	
	
	
	
	

	3.1D
	Normal - Nosewheel and rudder steering.
	
	
	
	
	
	
	
	
	
	
	

	3.1E
	Normal - Crosswind (max demonstrated).
	
	
	
	
	
	
	
	
	
	
	

	3.1F
	Normal - Special performance (reduced V1, max de-rate, short field).
	
	
	
	
	
	
	
	
	
	
	

	3.1G
	Normal - Low visibility take-off.
	
	
	
	
	
	
	
	
	
	
	

	3.1H
	Normal - Gear, flap, leading edge devices.
	
	
	
	
	
	
	
	
	
	
	

	3.1I
	Normal - Contaminated runway operation.
	
	
	
	
	
	
	
	
	
	
	

	3.1J
	Normal - Other.
	
	
	
	
	
	
	
	
	
	
	

	3.2A
	Abnormal - Rejected take-off.
	
	
	
	
	
	
	
	
	
	
	

	3.2B
	Abnormal - Rejected special performance.
	
	
	
	
	
	
	
	
	
	
	

	3.2C
	Abnormal - Engine failure at critical point, continued T/O.
	
	
	
	
	
	
	
	
	
	
	

	3.2D
	Abnormal - With wind shear.
	
	
	
	
	
	
	
	
	
	
	

	3.2E
	Abnormal - Flight control system failures, reconfig modes.
	
	
	
	
	
	
	
	
	
	
	

	3.2F
	Abnormal - Rejected, brake fade.
	
	
	
	
	
	
	
	
	
	
	

	3.2G
	Abnormal - Rejected, contaminated runway.
	
	
	
	
	
	
	
	
	
	
	

	3.2H
	Abnormal - Other.
	
	
	
	
	
	
	
	
	
	
	

	4. Climb

	4.1
	Normal climb.
	
	
	
	
	
	
	
	
	
	
	

	4.2
	One or more engines inoperative.
	
	
	
	
	
	
	
	
	
	
	

	4.3
	Other.
	
	
	
	
	
	
	
	
	
	
	

	5. Cruise

	5.1
	Performance characteristics (speed vs power).
	
	
	
	
	
	
	
	
	
	
	

	5.2
	High altitude handling.
	
	
	
	
	
	
	
	
	
	
	

	5.3
	High Mach number handling and recovery (trim change).
	
	
	
	
	
	
	
	
	
	
	

	5.4
	Overspeed warning (Vmo/Mmo).
	
	
	
	
	
	
	
	
	
	
	

	5.5
	High IAS handling.
	
	
	
	
	
	
	
	
	
	
	

	6. Manoeuvres

	6.1A
	Approach to stalls, stall warning, buffet (all configs).
	
	
	
	
	
	
	
	
	
	
	

	6.1B
	Approach to stalls including full stall and g-break (all configs).
	
	
	
	
	
	
	
	
	
	
	

	6.1C
	Upset prevention and recovery within FSTD validation envelope.
	
	
	
	
	
	
	
	
	
	
	

	6.2
	Flight envelope protection (high AoA, bank limit, overspeed).
	
	
	
	
	
	
	
	
	
	
	

	6.3
	Turns with/without speedbrake/spoilers.
	
	
	
	
	
	
	
	
	
	
	

	6.4
	Normal and standard rate turns.
	
	
	
	
	
	
	
	
	
	
	

	6.5
	Steep turns.
	
	
	
	
	
	
	
	
	
	
	

	6.6
	Performance turn.
	
	
	
	
	
	
	
	
	
	
	

	6.7
	In-flight engine shutdown and restart.
	
	
	
	
	
	
	
	
	
	
	

	6.8
	Manoeuvring with engine(s) inoperative.
	
	
	
	
	
	
	
	
	
	
	

	6.9
	Specific flight characteristics (e.g. direct lift control).
	
	
	
	
	
	
	
	
	
	
	

	6.10
	Flight control system failures, reconfig, manual reversion.
	
	
	
	
	
	
	
	
	
	
	

	6.11
	Other.
	
	
	
	
	
	
	
	
	
	
	

	7. Descent

	7.1
	Normal descent.
	
	
	
	
	
	
	
	
	
	
	

	7.2
	Max rate descent (clean/speedbrake).
	
	
	
	
	
	
	
	
	
	
	

	7.3
	Descent with autopilot.
	
	
	
	
	
	
	
	
	
	
	

	7.4
	Descent with flight control failures, reconfig, manual reversion.
	
	
	
	
	
	
	
	
	
	
	

	7.5
	Other.
	
	
	
	
	
	
	
	
	
	
	

	8. Instrument Approaches

	8.1A
	Precision - PAR.
	
	
	
	
	
	
	
	
	
	
	

	8.1B(i)
	CAT I - Manual with/without flight director including landing.
	
	
	
	
	
	
	
	
	
	
	

	8.1B(ii)
	CAT I - Autopilot/auto throttle coupled approach, manual landing.
	
	
	
	
	
	
	
	
	
	
	

	8.1B(iii)
	CAT I - Manual to DH, G/A all engines.
	
	
	
	
	
	
	
	
	
	
	

	8.1B(iv)
	CAT I - One engine out approach to DH and G/A.
	
	
	
	
	
	
	
	
	
	
	

	8.1B(v)a
	CAT I - Below minima with crosswind (max demonstrated).
	
	
	
	
	
	
	
	
	
	
	

	8.1B(v)b
	CAT I - Below minima with wind shear.
	
	
	
	
	
	
	
	
	
	
	

	8.1B(vi)
	CAT I - Autopilot coupled, OEI to DH and G/A.
	
	
	
	
	
	
	
	
	
	
	

	8.1B(vii)
	CAT I - Approach/landing with min/standby electrical power.
	
	
	
	
	
	
	
	
	
	
	

	8.1C(i)
	CAT II - Auto coupled to DH and landing.
	
	
	
	
	
	
	
	
	
	
	

	8.1C(ii)
	CAT II - Auto coupled to DH and G/A.
	
	
	
	
	
	
	
	
	
	
	

	8.1C(iii)
	CAT II - Auto coupled to DH and manual G/A.
	
	
	
	
	
	
	
	
	
	
	

	8.1C(iv)
	CAT II - Auto coupled/auto throttle published approach.
	
	
	
	
	
	
	
	
	
	
	

	8.1D(i)
	CAT III - Auto coupled to land and rollout.
	
	
	
	
	
	
	
	
	
	
	

	8.1D(ii)
	CAT III - Auto coupled to DH/Alert Height and G/A.
	
	
	
	
	
	
	
	
	
	
	

	8.1D(iii)
	CAT III - Auto coupled to land and rollout, OEI.
	
	
	
	
	
	
	
	
	
	
	

	8.1D(iv)
	CAT III - Auto coupled to DH/Alert Height and G/A, OEI.
	
	
	
	
	
	
	
	
	
	
	

	8.1E(i)
	Auto coupled approach - with generator failure.
	
	
	
	
	
	
	
	
	
	
	

	8.1E(ii)
	Auto coupled approach - with 10 kts tail wind.
	
	
	
	
	
	
	
	
	
	
	

	8.1E(iii)
	Auto coupled approach - with 10 kts crosswind.
	
	
	
	
	
	
	
	
	
	
	

	8.2A
	Non-precision - NDB.
	
	
	
	
	
	
	
	
	
	
	

	8.2B
	Non-precision - VOR, VOR/DME, VOR/TAC.
	
	
	
	
	
	
	
	
	
	
	

	8.2C
	Non-precision - RNAV (GNSS).
	
	
	
	
	
	
	
	
	
	
	

	8.2D
	Non-precision - ILS LLZ (LOC), LLZ(LOC)/BC.
	
	
	
	
	
	
	
	
	
	
	

	8.2E
	Non-precision - ILS offset localizer.
	
	
	
	
	
	
	
	
	
	
	

	8.2F
	Non-precision - Direction finding facility.
	
	
	
	
	
	
	
	
	
	
	

	8.2G
	Non-precision - Surveillance radar.
	
	
	
	
	
	
	
	
	
	
	

	9. Visual Approaches & Landings

	9.1
	Normal approach and landing, all engines.
	
	
	
	
	
	
	
	
	
	
	

	9.2
	Approach/landing with engine(s) inoperative.
	
	
	
	
	
	
	
	
	
	
	

	9.3
	Gear, flaps/slats, speedbrakes (normal/abnormal).
	
	
	
	
	
	
	
	
	
	
	

	9.4
	Crosswind approach and landing (max demonstrated).
	
	
	
	
	
	
	
	
	
	
	

	9.5
	Approach with wind shear.
	
	
	
	
	
	
	
	
	
	
	

	9.6
	Approach/landing with flight control failures, reconfig.
	
	
	
	
	
	
	
	
	
	
	

	9.7A
	Longitudinal trim malfunction.
	
	
	
	
	
	
	
	
	
	
	

	9.7B
	Lateral-directional trim malfunction.
	
	
	
	
	
	
	
	
	
	
	

	9.8
	Approach/landing with standby electrical/hydraulic power.
	
	
	
	
	
	
	
	
	
	
	

	9.9
	Approach/landing from circling conditions.
	
	
	
	
	
	
	
	
	
	
	

	9.10
	Approach/landing from visual traffic pattern.
	
	
	
	
	
	
	
	
	
	
	

	9.11
	Approach/landing from non-precision approach.
	
	
	
	
	
	
	
	
	
	
	

	9.12
	Approach/landing from precision approach.
	
	
	
	
	
	
	
	
	
	
	

	9.13
	Approach procedures with vertical guidance (APV), e.g. SBAS.
	
	
	
	
	
	
	
	
	
	
	

	9.14
	Other.
	
	
	
	
	
	
	
	
	
	
	

	10. Missed Approach

	10.1
	All engines go-around.
	
	
	
	
	
	
	
	
	
	
	

	10.2
	One or more engine(s) out go-around.
	
	
	
	
	
	
	
	
	
	
	

	10.3
	With flight control failures, reconfig, manual reversion.
	
	
	
	
	
	
	
	
	
	
	

	11. Post Landing Ops

	11.1A
	Spoiler operation.
	
	
	
	
	
	
	
	
	
	
	

	11.1B
	Reverse thrust operation.
	
	
	
	
	
	
	
	
	
	
	

	11.1C
	Directional control and ground handling, with/without reverse.
	
	
	
	
	
	
	
	
	
	
	

	11.1D
	Reduction of rudder effectiveness with increased reverse thrust (rear pod-mounted).
	
	
	
	
	
	
	
	
	
	
	

	11.1E
	Brake and anti-skid (dry, wet, icy).
	
	
	
	
	
	
	
	
	
	
	

	11.1F
	Brake operation with auto-braking system.
	
	
	
	
	
	
	
	
	
	
	

	11.1G
	Other.
	
	
	
	
	
	
	
	
	
	
	

	12. Any Flight Phase - Systems

	12.1A
	Air conditioning and pressurisation (ECS).
	
	
	
	
	
	
	
	
	
	
	

	12.1B
	De-icing / anti-icing.
	
	
	
	
	
	
	
	
	
	
	

	12.1C
	Auxiliary powerplant / APU.
	
	
	
	
	
	
	
	
	
	
	

	12.1D
	Communications.
	
	
	
	
	
	
	
	
	
	
	

	12.1E
	Electrical.
	
	
	
	
	
	
	
	
	
	
	

	12.1F
	Fire and smoke detection and suppression.
	
	
	
	
	
	
	
	
	
	
	

	12.1G
	Flight controls (primary/secondary).
	
	
	
	
	
	
	
	
	
	
	

	12.1H
	Fuel/oil, hydraulic, pneumatic.
	
	
	
	
	
	
	
	
	
	
	

	12.1I
	Landing gear.
	
	
	
	
	
	
	
	
	
	
	

	12.1J
	Oxygen.
	
	
	
	
	
	
	
	
	
	
	

	12.1K
	Powerplant.
	
	
	
	
	
	
	
	
	
	
	

	12.1L
	Airborne radar.
	
	
	
	
	
	
	
	
	
	
	

	12.1M
	Autopilot and flight director.
	
	
	
	
	
	
	
	
	
	
	

	12.1N
	Collision avoidance (GPWS, TCAS).
	
	
	
	
	
	
	
	
	
	
	

	12.1O
	Flight control computers including stability and control augmentation.
	
	
	
	
	
	
	
	
	
	
	

	12.1P
	Flight display systems.
	
	
	
	
	
	
	
	
	
	
	

	12.1Q
	Flight management computers.
	
	
	
	
	
	
	
	
	
	
	

	12.1R
	Head-up guidance, head-up displays.
	
	
	
	
	
	
	
	
	
	
	

	12.1S
	Navigation systems.
	
	
	
	
	
	
	
	
	
	
	

	12.1T
	Stall warning/avoidance.
	
	
	
	
	
	
	
	
	
	
	

	12.1U
	Wind shear avoidance equipment.
	
	
	
	
	
	
	
	
	
	
	

	12.1V
	Automatic landing aids.
	
	
	
	
	
	
	
	
	
	
	

	12.2A
	Holding.
	
	
	
	
	
	
	
	
	
	
	

	12.2B
	Air hazard avoidance (traffic, weather).
	
	
	
	
	
	
	
	
	
	
	

	12.2C
	Wind shear.
	
	
	
	
	
	
	
	
	
	
	

	12.3A
	Engine and systems shutdown.
	
	
	
	
	
	
	
	
	
	
	

	12.3B
	Parking brake operation.
	
	
	
	
	
	
	
	
	
	
	

	12.3C
	Other as appropriate including effects of wind.
	
	
	
	
	
	
	
	
	
	
	

	13. Visual System - Content (C/D)

	13.1A
	Two parallel runways and one crossing runway displayed simultaneously.
	
	
	
	
	
	
	
	
	
	
	

	13.1B
	Runway threshold elevations/locations modelled for system correlation.
	
	
	
	
	
	
	
	
	
	
	

	13.1C
	Representative airport buildings, structures and lighting.
	
	
	
	
	
	
	
	
	
	
	

	13.1D
	One useable gate at appropriate height.
	
	
	
	
	
	
	
	
	
	
	

	13.1E
	Representative moving and static gate clutter.
	
	
	
	
	
	
	
	
	
	
	

	13.1F
	Representative gate/apron markings and lighting.
	
	
	
	
	
	
	
	
	
	
	

	13.1G
	Representative runway markings, lighting, signage, wind sock.
	
	
	
	
	
	
	
	
	
	
	

	13.1H
	Representative taxiway markings, lighting, signage for taxi route.
	
	
	
	
	
	
	
	
	
	
	

	13.1I
	Representative moving and static ground traffic.
	
	
	
	
	
	
	
	
	
	
	

	13.1J
	Representative terrain and obstacles within 25 NM.
	
	
	
	
	
	
	
	
	
	
	

	13.1K
	Representative natural and cultural features within 25 NM.
	
	
	
	
	
	
	
	
	
	
	

	13.1L
	Representative moving airborne traffic.
	
	
	
	
	
	
	
	
	
	
	

	13.1M
	Appropriate approach lighting for VFR, non-precision, CAT I/II/III.
	
	
	
	
	
	
	
	
	
	
	

	13.1N
	Representative gate docking aids or marshaller.
	
	
	
	
	
	
	
	
	
	
	

	13. Visual System - Content (A/B)

	13.2A
	Representative airport runways and taxiways.
	
	
	
	
	
	
	
	
	
	
	

	13.2B
	Runway definition.
	
	
	
	
	
	
	
	
	
	
	

	13.2C
	Runway surface and markings.
	
	
	
	
	
	
	
	
	
	
	

	13.2D
	Lighting for runway in use including edge, centreline, and approach lights.
	
	
	
	
	
	
	
	
	
	
	

	13.2E
	Representative taxiway lights.
	
	
	
	
	
	
	
	
	
	
	

	13. Visual Scene Management & Feature Recognition

	13.3A
	Runway/approach lighting intensity representative for visibility set.
	
	
	
	
	
	
	
	
	
	
	

	13.3B
	Directionality of strobe, approach, edge, centreline, threshold, TDZ lights.
	
	
	
	
	
	
	
	
	
	
	

	13.4A
	Runway definition, strobes, approach/edge lights from 8 km (5 sm).
	
	
	
	
	
	
	
	
	
	
	

	13.4B
	Visual approach aids lights from 8 km (5 sm).
	
	
	
	
	
	
	
	
	
	
	

	13.4C
	Visual approach aids lights from 5 km (3 sm).
	
	
	
	
	
	
	
	
	
	
	

	13.4D
	Runway centreline lights and taxiway definition from 5 km (3 sm).
	
	
	
	
	
	
	
	
	
	
	

	13.4E
	Threshold and TDZ lights from 3 km (2 sm).
	
	
	
	
	
	
	
	
	
	
	

	13.4F
	Runway markings within range of landing lights (night) / resolution (day).
	
	
	
	
	
	
	
	
	
	
	

	13.4G
	Circling: runway of intended landing fades into view non-distractingly.
	
	
	
	
	
	
	
	
	
	
	

	13. Airport Model / Correlation / Scene Quality / Environment

	13.5A
	Terminal approach area: portrayal, lights, ramps, terrain, dynamic effects, illusions.
	
	
	
	
	
	
	
	
	
	
	

	13.6A
	Visual system compatibility with aerodynamic programming.
	
	
	
	
	
	
	
	
	
	
	

	13.6B
	Visual cues for sink rate/depth; runway perspective for approach path.
	
	
	
	
	
	
	
	
	
	
	

	13.6C
	Accurate environment portrayal relating to FSTD attitudes.
	
	
	
	
	
	
	
	
	
	
	

	13.6D
	Visual correlates with aeroplane systems (terrain, traffic, weather, HGS).
	
	
	
	
	
	
	
	
	
	
	

	13.6E
	Representative visual effects for each ownship external light.
	
	
	
	
	
	
	
	
	
	
	

	13.6F
	Rain removal device visual effects.
	
	
	
	
	
	
	
	
	
	
	

	13.7A
	Surfaces/textural cues free from aliasing.
	
	
	
	
	
	
	
	
	
	
	

	13.7B
	Full colour realistic textural cues.
	
	
	
	
	
	
	
	
	
	
	

	13.7C
	Light points free from jitter, smearing, streaking.
	
	
	
	
	
	
	
	
	
	
	

	13.7D
	Occulting demonstrated through each channel.
	
	
	
	
	
	
	
	
	
	
	

	13.7E
	Min 10 levels of occulting through each channel.
	
	
	
	
	
	
	
	
	
	
	

	13.8A
	Scene matches surface contaminants (wet reflections, snow-obscured lights).
	
	
	
	
	
	
	
	
	
	
	

	13.8B
	Special weather: precipitation near thunderstorm below 2000 ft within 16 km.
	
	
	
	
	
	
	
	
	
	
	

	13.8C
	In-cloud effects: variable density, speed cues, ambient changes.
	
	
	
	
	
	
	
	
	
	
	

	13.8D
	Multiple cloud layers (few/scattered/broken/overcast).
	
	
	
	
	
	
	
	
	
	
	

	13.8E
	Gradual break-out to ambient visibility/RVR (20-200 ft transition).
	
	
	
	
	
	
	
	
	
	
	

	13.8F
	Visibility/RVR measured in distance below 2000 ft within 16 km.
	
	
	
	
	
	
	
	
	
	
	

	13.8G
	Patchy fog giving variable RVR effect.
	
	
	
	
	
	
	
	
	
	
	

	13.8H
	Fog effects on aerodrome lighting (halos, defocus).
	
	
	
	
	
	
	
	
	
	
	

	13.8I
	Ownship lighting in reduced visibility (glare from lights, strobes, beacons).
	
	
	
	
	
	
	
	
	
	
	

	13.8J
	Blowing snow/sand across runway selectable from IOS.
	
	
	
	
	
	
	
	
	
	
	

	13.9A
	IOS controls: cloud base, density, visibility, RVR.
	
	
	
	
	
	
	
	
	
	
	

	13.9B
	IOS controls: airport/aerodrome selection.
	
	
	
	
	
	
	
	
	
	
	

	13.9C
	IOS controls: airport lighting including variable intensity.
	
	
	
	
	
	
	
	
	
	
	

	13.9D
	IOS controls: dynamic effects including ground and flight traffic.
	
	
	
	
	
	
	
	
	
	
	

	13.10
	Night visual scene capability.
	
	
	
	
	
	
	
	
	
	
	

	13.11
	Twilight visual scene capability.
	
	
	
	
	
	
	
	
	
	
	

	13.12
	Daylight visual scene capability.
	
	
	
	
	
	
	
	
	
	
	

	14. Motion Effects

	14.1
	Runway rumble, oleo deflections, ground speed, uneven runway, centreline lights.
	
	
	
	
	
	
	
	
	
	
	

	14.2
	Ground buffets from spoiler/speedbrake extension and thrust reversal.
	
	
	
	
	
	
	
	
	
	
	

	14.3
	Bumps associated with landing gear.
	
	
	
	
	
	
	
	
	
	
	

	14.4
	Buffet during gear extension and retraction.
	
	
	
	
	
	
	
	
	
	
	

	14.5
	Airborne buffet from flap/spoiler extension; approach to stall buffet.
	
	
	
	
	
	
	
	
	
	
	

	14.6
	Approach to stall buffet and stall buffet (where applicable).
	
	
	
	
	
	
	
	
	
	
	

	14.7
	Touchdown cues for main and nose gear.
	
	
	
	
	
	
	
	
	
	
	

	14.8
	Nose wheel scuffing.
	
	
	
	
	
	
	
	
	
	
	

	14.9
	Thrust effect with brakes set.
	
	
	
	
	
	
	
	
	
	
	

	14.10
	Mach and manoeuvre buffet.
	
	
	
	
	
	
	
	
	
	
	

	14.11
	Tyre failure dynamics.
	
	
	
	
	
	
	
	
	
	
	

	14.12
	Engine malfunction and engine damage.
	
	
	
	
	
	
	
	
	
	
	

	14.13
	Tail strikes and pod strikes.
	
	
	
	
	
	
	
	
	
	
	

	15. Sound System

	15.1A
	Precipitation sound.
	
	
	
	
	
	
	
	
	
	
	

	15.1B
	Rain removal equipment sound.
	
	
	
	
	
	
	
	
	
	
	

	15.1C
	Significant aeroplane noises during normal operations.
	
	
	
	
	
	
	
	
	
	
	

	15.1D
	Abnormal operations sound cues (fire bell, overspeed, stall, config warning).
	
	
	
	
	
	
	
	
	
	
	

	15.1E
	Crash sound when landed in excess of limitations.
	
	
	
	
	
	
	
	
	
	
	

	15.1F
	Significant engine/propeller noise during normal operations.
	
	
	
	
	
	
	
	
	
	
	

	16. Special Effects

	16.1A
	Representative brake failure dynamics (antiskid) and decreased brake efficiency.
	
	
	
	
	
	
	
	
	
	
	

	16.2A
	Effects of airframe and engine icing.
	
	
	
	
	
	
	
	
	
	
	

	17. Others

	17.1
	GPS.
	
	
	
	
	
	
	
	
	
	
	

	17.2
	ETOPS / EDTO Capabilities.
	
	
	
	
	
	
	
	
	
	
	

	17.3A
	UPRT: Upset prevention and recovery within FSTD validation envelope.
	
	
	
	
	
	
	
	
	
	
	

	17.3B
	UPRT: Instructor operating station control and briefing.
	
	
	
	
	
	
	
	
	
	
	

	17.3C
	Icing indicators (engine and airframe).
	
	
	
	
	
	
	
	
	
	
	




	Audit Summary

	Total Items
	66
	Evaluated
	0
	SAT (S)
	0

	UNSAT (U)
	0
	OBS (O)
	0
	





	
	Findings / Observations No.
	Comments
	Deadline
	Classification

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	

	9
	
	
	
	

	10
	
	
	
	

	11
	
	
	
	

	12
	
	
	
	

	13
	
	
	
	

	14
	
	
	
	

	15
	
	
	
	



	Classification of Findings (ORA.GEN.150)

	Level 1
	A level 1 finding shall be issued by the CAAT when any significant non-compliance is detected with the applicable requirements, with the organisation’s procedures and manuals or with the terms of an approval, or certificate which lowers safety or seriously endangers flight safety.

	Level 2
	A level 2 finding shall be issued by the CAAT when any non-compliance is detected with the applicable requirement, with the organisation’s procedures and manuals or with the terms of an approval, or certificate which could lower safety or seriously hazards flight safety

	OBS
	Observation is opportunity for improvement which is minor gap, mostly documented and implemented. The management system that may be weak, cumbersome, redundant, overly complex, or in some other manner, may, in the opinion of the auditor, offer an opportunity for an organisation to improve its current status. An observation is not subject to any corrective actions unless it is accepted by auditee for improvement.



	Lead Auditor Signature:
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	Date: 
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