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Checklist Number:                             OPS-TCFOI-306                                                              
Checklist Name:                         OPS - Helicopter Main AOC                       
Applicability:                                                                                          
Location:                                                 Date:                                       





	No
	Subject
	Reference
	S
	U
	N/A
	Comment

	0
	Preliminary
	
	
	
	
	

	0.1
	Operator Name 
	
	
	
	
	

	0.2
	Main Base of Operation
	
	
	
	
	

	0.3
	Helicopter Types Operated
	
	
	
	
	

	0.4
	Name of CAAT POI
	
	
	
	
	

	0.5
	Name of CAAT FOI
	
	
	
	
	

	0.6
	Name of CAAT OMI
	
	
	
	
	

	0.7
	Name of CAAT DGI
	
	
	
	
	

	0.8
	Name of CAAT AWI
	
	
	
	
	

	0.9
	Date of Inspection
	
	
	
	
	

	[bookmark: _Hlk147133393]1
	SUBPART A: GENERAL REQUIREMENTS
	
	
	
	
	

	
	SECTION 1 Motor-powered aircraft
	
	
	
	
	

	1.1
	Does the manual include commander responsibilities for:
(a) Compliance with CAT.GEN.MPA.105(a);
(b) Remaining at station during emergencies requiring immediate action;
(c) Submitting ACAS reports to CAAT;
(d) Submitting bird strike reports to CAAT; and
(e) Reporting hazardous weather to ATS?
	CAT.GEN.MPA.105
	
	
	
	

	1.2
	Does the manual describe that a helicopter rotor shall only be turned under power for the purpose of flight, with a qualified pilot at the controls?
	CAT.GEN.MPA.130
	
	
	
	

	1.3
	Does the manual describe procedures for the carriage of sporting weapons and ammunition, including:
(a) Procedure for reporting sporting weapons to the operator;
(b) Stowage in a location inaccessible to passengers during flight; and
(c) Carriage in checked baggage in accordance with the Technical Instructions?
	CAT.GEN.MPA.160
	
	
	
	

	1.4
	Does the manual describe procedures for the carriage of sporting weapons and ammunition alleviations for helicopters with an MCTOM of 3 175 kg or less operated by day under VFR, where inaccessible stowage during flight is impracticable?
	CAT. GEN. MPA. 161
	
	
	
	

	2
	SUBPART B: OPERATING PROCEDURES
	
	
	
	
	

	2.1
	Does the manual describe procedures for the use of ATS, including:
(a) compliance with applicable rules of the air for all flights; and
(b) coordination of ATS flight plan changes with the appropriate ATS unit before transmission to the aircraft, when practicable?
	CAT.OP.MPA.100
	
	
	
	

	2.2
	Does the manual describe procedures for the use of aerodromes, heliports, and operating sites, including:
(a) Use of adequate aerodromes and heliports for the intended aircraft and operations;
(b) Criteria for determining site adequacy for each operation;
(c) Site surveys conducted by a competent person;
(d) Inclusion of site diagrams, photographs, and descriptions in the operations manual;
(e) Pilot assessment procedures for non-pre-surveyed sites from the air; and
(d) Restriction of night operations to non-pre-surveyed sites, except as permitted by SPA.HEMS.125(b)(4)?
	CAT.OP.MPA.105;
AMC1 CAT.OP.MPA.105
	
	
	
	

	2.3
	Does the manual describe helicopter noise abatement procedures, including:
(a) Minimising helicopter noise during take-off and landing; and
(b) Ensuring safety takes priority over noise abatement?
	CAT.OP.MPA.131
	
	
	
	

	2.4
	Does the manual describe procedures for helicopter routes and areas of operation, including:
(a) Availability of safe forced-landing surfaces for performance class 3 operations, unless approved under CAT.POL.H.420; and
(b) coastal transit procedures for performance class 3 operations, including corridor width and required equipment appropriate to prevailing conditions?
	CAT.OP.MPA.137
	
	
	
	

	2.5
	Does the manual describe that an operational flight plan shall be completed for each intended flight based on considerations of aircraft performance, other operating limitations and relevant expected conditions on the route to be followed and at the aerodromes/operating sites concerned.
	CAT.OP.MPA.175
	
	
	
	

	2.6
	Does the manual describe procedures for fuel/energy scheme, including: 
(a) Planning and in-flight re-planning policy;
(b) In-flight fuel/energy management policy;
(c) Appropriate for the type(s) of operation performed;
(d) Corresponds to the capability of the operator to support its implementation; and
(e) Require prior approval by the CAAT?
	CAT.OP.MPA.190
	
	
	
	

	2.7
	Does the manual describe procedures for fuel/energy scheme, including: 
(a) Carrying sufficient fuel/energy for the planned flight and foreseeable deviations;
(b) Pre-flight usable fuel/energy calculations;
(c) In-flight re-planning procedures; and
(d) Planning minima, safety margins, and alternate aerodrome selection?
	CAT.OP.MPA.191;
AMC1 CAT.OP.MPA.191(b)&(c)
	
	
	
	

	2.8
	Does the manual describe procedures for the selection of aerodromes and operating sites for helicopters, including:
(a) Selection of a take-off alternate within one hour flying time at normal cruising speed;
(b) Availability of two safe landing options for each IFR flight;
(c) Application of safety margins for possible weather deterioration; and
(d) Availability of adequate means to navigate to and land at the destination or alternate aerodrome/site?
	CAT.OP.MPA.192
	
	
	
	

	2.9
	Does the manual describe procedures for fuel/energy scheme, including: 
(a) Procedure for in-flight fuel/energy checks and fuel/energy management are performed;
(b) Monitoring the amount of usable fuel/energy remaining on board;
(c) Advise air traffic control (ATC) of a ‘minimum fuel/energy’ state by declaring ‘MINIMUM FUEL’; and
(d) Declare a situation of ‘fuel/energy emergency’ by broadcasting ‘MAYDAY MAYDAY MAYDAY FUEL’?
	CAT.OP.MPA.195;
AMC1 CAT.OP.MPA.195
	
	
	
	

	2.10
	Does the manual describe procedures for special refueling or defueling, including: 
(a) Performed a risk assessment;
(b)  Special Refueling or defueling procedures; and
(c) Training programme for its personnel involved in such operations.
	CAT.OP.MPA.200;
AMC3 CAT.OP.MPA.200
	
	
	
	

	2.11
	Does the manual describe that each flight crew member required to be on duty in the flight crew compartment shall wear a headset with boom microphone, or equivalent, and use it as the primary device to communicate with ATS.
	CAT.OP.MPA.216
	
	
	
	

	2.12
	Does the manual describe that when operating a helicopter over water in performance class 3, account is taken of the duration of the flight and conditions to be encountered when deciding if life-jackets are to be worn by all occupants.
	CAT.OP.MPA.235
	
	
	
	

	2.13
	Does the manual describe procedures for meteorological conditions, including:
(a) Verification that forecast weather at the destination and alternate aerodrome(s) is at or above planning minima;
(b) Use of the latest available weather information before continuing IFR flights to the destination; and 
(c) Ensuring meteorological conditions are suitable for VFR operations before commencing flight?
	CAT.OP.MPA.245
	
	
	
	

	2.14
	Does the manual describe meteorological procedures for helicopters, including:
(a) minimum cloud ceiling requirements for VFR overwater flights out of sight of land; and
(b) limiting operations to helidecks or elevated FATOs when mean wind speed is below 60 kt?
	CAT.OP.MPA.247
	
	
	
	

	2.15
	Does the manual describe that before commencing an approach to land, the commander shall be satisfied that according to the information available to him or her, the weather at the aerodrome and the condition of the final approach and take-off area (FATO) intended to be used would not prevent a safe approach, landing or missed approach, having regard to the performance information contained in the operations manual (OM)?
	CAT.OP.MPA.301
	
	
	
	

	2.16
	Does the manual describe procedures for commencement and continuation of approach, including:
(a) Discontinuing instrument approaches when reported RVR is below applicable minima;
(b) Executing a missed approach if required visual reference is not established by DA/H or MDA/H;
(c) Conducting a prompt go-around if visual reference is lost after DA/H or MDA/H; and
(d) Continuation of approach using CMV when RVR is unavailable and reported visibility is below minima?
	CAT.OP.MPA.305
	
	
	
	

	2.17
	Does the manual describe that the operator shall make available to the CAAT the hours flown for each helicopter operated during the previous calendar year?
	CAT.OP.MPA.315
	
	
	
	

	3
	SUBPART C: AIRCRAFT PERFORMANCE AND OPERATING LIMITATIONS
	
	
	
	
	

	
	SECTION 2 Helicopters
	
	
	
	
	

	[bookmark: _Hlk147135986]
	CHAPTER 1 General requirements
	
	
	
	
	

	3.1
	Does the manual describe helicopter performance class requirements, including:
(a) Use of performance class 1 in congested hostile environments, except PIS operations under CAT.POL.H.225;
(b) Use of performance class 1 or 2 for helicopters with a MOPSC of 10–19; and
(c) Use of performance class 1, 2, or 3 for helicopters with a MOPSC of 9 or less?
	CAT.POL.H.100
	
	
	
	

	3.2
	Does the manual describe helicopter performance class requirements, including: 
(a) The mass (weight and balance) calculation of the helicopter;
(b) Use of performance data contained in the AFM; and
(c) Method for analyzing the effects of helicopter configuration, environmental conditions, and any systems that adversely affect performance?
	CAT.POL.H.105
	
	
	
	

	3.3
	Does the manual describe obstacle accountability, including: 
(a) Consideration of an obstacle located beyond the FATO, in the take-off flight path, or the missed approach flight path; and
(b) Consideration of obstacles located in the back-up or lateral transition area for take-off using a back-up or a lateral transition procedure?
	CAT.POL.H.110
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	CHAPTER 2 Performance class 1
	
	
	
	
	

	3.4
	General:
Helicopters operated in performance class 1 shall be certified in category A or equivalent as determined by the CAAT.
	CAT.POL.H.200
	
	
	
	

	3.5
	Does the manual describe take-off procedures, including:
(a) Calculation of maximum take-off mass in accordance with the AFM;
(b) Consideration of CAT.POL.H.105(c) parameters at the departure site;
(c) Conducting take-off up to the TDP in sight of the surface to allow a rejected take-off; and
(d) Obstacle clearance for backup or lateral transition procedures following critical engine failure at or before the TDP?
	CAT.POL.H.205;
AMC1 CAT.POL.H.205(b)(4);
AMC1 CAT.POL.H.205(e);

	
	
	
	

	3.6
	Does the manual describe take-off flight path procedures, including:
(a) Ensuring adequate obstacle clearance along the take-off flight path; and
(b) Accounting for bank angle effects when turns greater than 15° are performed?
	CAT.POL.H.210
	
	
	
	

	3.7
	Does the manual describe en-route procedures with the critical engine inoperative, including:
(a) Compliance with CAT.POL.H.215 performance throughout the route;
(b) assuming critical engine failure at the most critical point;
(c) Consideration of wind effects on the flight path; and
(d) Planning for fuel jettisoning, where applicable?
	CAT.POL.H.215
	
	
	
	

	3.8
	Does the manual describe landing procedures, including:
(a) Compliance with AFM maximum landing mass limits;
(b) Calculation of the landing decision point (LDP) to ensure safe landing or balked landing obstacle clearance;
(c) Consideration of estimated landing time at the destination or alternate site; and
(d) Conducting the landing from LDP to touchdown in sight of the surface?
	CAT.POL.H.220
	
	
	
	

	3.9
	Does the manual describe procedures for helicopter operations to/from a public interest site (PIS), including: (a) site-specific procedures to minimise risks to occupants and persons on the surface in the event of engine failure during take-off and landing?
	CAT.POL.H.225;
AMC1 CAT.POL.H.225(a)(5)
	
	
	
	

	
	CHAPTER 3 Performance class 2
	
	
	
	
	

	3.10
	General:
Helicopters operated in performance class 2 shall be certified in category A.
	CAT.POL.H.300
	
	
	
	

	3.11
	Does the manual describe procedures for operations without an assured safe forced landing capability, including:
(a) Operations conducted only with CAAT approval;
completion of a helicopter- and operation-specific risk assessment; and
(b) Implementation of a usage monitoring system (UMS)?
	CAT.POL.H.305;
AMC1 CAT.POL.H.305(a);
AMC1 CAT.POL.H.305(b);
AMC2 CAT.POL.H.305(b)
	
	
	
	

	3.12
	Does the manual describe take-off procedures, including:
(a) Take-off mass limits for achieving a 150 ft/min climb rate at 1 000 ft with the critical engine inoperative;
(b) Conducting take-off to allow a safe forced landing until safe flight continuation is possible;
(c) Compliance with AFM AEO OGE hover mass limits; and
(d) Helideck take-off mass considerations, including procedure, deck-edge miss, and drop-down with critical engine inoperative?
	CAT.POL.H.310;
AMC1 CAT.POL.H.310(c)(2) and CAT.POL.H.325(c)(2)
	
	
	
	

	3.13
	Does the manual describe that take-off from the defined point after take-off (DPATO) or, as an alternative, no later than 200 ft above the take-off surface, with the critical engine inoperative.
	CAT.POL.H.315
	
	
	
	

	3.14
	En-route — critical engine inoperative
The requirement of CAT.POL.H.215 shall be complied with.
	CAT.POL.H.320
	
	
	
	

	3.15
	Does the manual describe landing procedures, including:
(a) Landing mass limits for achieving a 150 ft/min climb rate at 1 000 ft with the critical engine inoperative;
(b) Capability to perform a balked landing in accordance with CAT.POL.H.315;
(c) Capability to perform a safe forced landing where applicable;
(d) Compliance with AFM AEO OGE hover mass limits;
(e) Helideck landing mass considerations, including procedure and drop-down with the critical engine inoperative; and
(f) Conducting the final landing phase in sight of the surface when a balked landing is no longer possible?
	CAT.POL.H.325
	
	
	
	

	
	CHAPTER 4 Performance class 3
	
	
	
	
	

	3.16
	Does the manual describe performance class 3 operational requirements, including:
(a) Certification in category A/equivalent or category B;
operations limited to non-hostile environments, except under CAT.POL.H.420;
(b) Operations without assured safe forced landing 
(c) Capability only when approved under CAT.POL.H.305; and
(d) Prohibition of night operations out of sight of the surface?
	CAT.POL.H.400
	
	
	
	

	3.17
	Does the manual describe take-off procedures, including:
(a) Take-off mass limited to the lower of the MCTOM or AFM performance limits;
(b) Maximum take-off mass for AEO hover in ground effect;
(c) Maximum take-off mass for AEO hover out of ground effect; and
(d) Capability to perform a safe forced landing following engine failure, except as permitted by CAT.POL.H.400(b)?
	CAT.POL.H.405
	
	
	
	

	3.18
	Does the manual describe en-route procedures, including:
(a) Capability to continue along the planned route or diversion above minimum flight altitude with all engines operating at maximum continuous power; and
(b) Capability to perform a safe forced landing following engine failure, except as permitted by CAT.POL.H.420?
	CAT.POL.H.410
	
	
	
	

	3.19
	Does the manual describe landing procedures, including:
(a) Landing mass limits within the maximum certified landing mass;
(b) Maximum landing mass for AEO hover in ground effect;
(c) Maximum landing mass for AEO hover out of ground effect; and
(d) Capability to perform a safe forced landing following engine failure, except as permitted by CAT.POL.H.400(b)?
	CAT.POL.H.415
	
	
	
	

	3.20
	Does the manual describe procedures for helicopter operations over hostile environments outside congested areas, including:
)a) conducting safety risk assessments appropriate to the operation and flight conditions;
limiting operations to areas and conditions specified in the approval; and
(b) operations conducted only with approval in accordance with CAT.POL.H.305(b)?

Note: Operations over non-congested hostile environments without safe forced landing capability, using turbine-powered helicopters with an MOPSC of 6 or less, require CAAT approval
	CAT.POL.H.420;
AMC1 CAT.POL.H.420
	
	
	
	

	
	SECTION 3 Mass and balance
	
	
	
	
	

	
	CHAPTER 1 Motor-powered aircraft
	
	
	
	
	

	3.21
	Does the manual describe procedures for mass, balance, and loading, including:
(a) Compliance with AFM loading, mass, and CG limitations;
(b) Aircraft weighing before initial service and at CAAT-approved intervals;
(c) Weighing by the manufacturer or an approved maintenance organisation;
(d) Determination of dry operating mass using actual or standard masses;
(e) Determination of traffic load using standard passenger and baggage masses;
(f) Establishment of standard passenger and checked baggage masses;
(g) Determination of fuel mass using actual density and fuel density calculations;
(h) Loading procedures;
(i) Compliance with additional structural limits; and
(j) Methods used in the loading and mass and balance system?
	CAT.POL.MAB.100
	
	
	
	

	3.22
	Does the manual describe procedures for mass and balance data and documentation, including:
(a) Preparation of mass and balance data and documentation before each flight;
(b) Instructions and procedures for computerised mass and balance systems;
(c) Confirmation of loading by the person supervising the loading;
(d) Commander acceptance by signature or equivalent; and
(e) Procedures for last-minute load changes?
	CAT.POL.MAB.105
	
	
	
	



S = Satisfied
U= Unsatisfied   
N/A= Not Applicable
Comment= Description the detail of compliance or Non Compliance or other information
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