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	No
	Subject
	Reference
	S
	U
	N/A
	Comment

	1
	Preliminary (General Information) 
	
	
	
	
	

	1.1
	Name of Operator
	 
	
	
	
	

	1.2
	Date of Application
	
	
	
	
	

	1.3
	New Type or Variant to be added ( e.g. B787-9 ) 
	
	
	
	
	

	1.4
	Name of POI
	
	
	
	
	

	1.5
	Name of AWI
	
	
	
	
	

	1.6
	Date of Inspection
	
	
	
	
	

	2
	Operations (OPS)
	
	
	
	
	

	2.1
	Revised or updated Operations Manual Parts A, B, C and D as appropriate which incorporates the following information;
(a) new information 
(b) new guidance
(c) new instructions pertaining to the new aircraft type and reflects the current operating environment of the operator.
(d) Operations Manual Parts B for a new type which contains the following information;
· aircraft systems
· limitations
· performance
· normal and abnormal operating procedures for the aircraft.
	ORO.MLR.100
ORO.MLR.101
AMC1 ORO.MLR.100
	
	
	
	

	2.2
	A Minimum Equipment List (MEL) for the new aircraft type which reflects the Master Minimum Equipment List approved by the State of Design and is tailored to the specific aircraft model and operating environment of the operator. 
(a)	This document requires signature and stamp of approval by the CAAT or his Designate. 
(b)	The MEL shall be approved by the CAAT after receiving recommendations from the Flight Operations Inspection, Airworthiness and Engineering Inspection Group.
Note:
1. For a new Type or variant check to the Operator shall produce a new MEL, use the MEL checklist to review it.
2. OPS and AIR should be coordinated to conduct the MEL checklist review in a timely manner.
	ORO.MLR.105
GM1 ORO.MLR.105(a)
AMC1/AMC2/GM1/GM2 ORO.MLR.105(c) to (j)















	
	
	
	

	2.3 
	A Configuration Deviation List (CDL) for the new aircraft type which contains information regarding flights with missing aircraft components.
	ORO.MLR.100
AMC3 ORO.MLR.100 (B) (4.3)
	
	
	
	

	2.4
	Check the effect on other manuals including:
(a) FCOM;
(b) QRH;
(c) Weight and Balance;
(d) SOP;
(e) AFM;
(f) FCTM;
(g) CCM;
(h) CCTM
(i) DGM; and
(j) Others
State the manuals that are affected in Comment Box
	ORO.MLR.100
ORO.MLR.101
AMC1 ORO.MLR.100
AMC3 ORO.MLR.100 (B) (6)





	
	
	
	

	2.5
	Checklist;
(a)	Normal checklist
(b)	Abnormal checklist
(c)	Emergency checklists for the new aircraft type, including abbreviated checklists for use in the cockpit. 
Note: These checklists must be approved by the CAAT or his Designate.
	ORO.GEN.110 (h)






	
	
	
	

	2.6
	Passenger briefing cards in English and other appropriate languages, demonstrate the new aircraft type.
	CAT.OP.MPA.170
AMC1 CAT.OP.MPA.170
	
	
	
	

	2.7
	A revised Cabin Crew Manual or other suitable reference for Cabin Crew concerning the following information;
(a) configuration of the new aircraft type
(b) location and operation of installed cabin equipment
duties and responsibilities during normal and abnormal operations.
	ORO.MLR.100








	
	
	
	

	2.8
	Airport Analysis charts or equivalent reference material for use by aircrew for determining maximum gross takeoff and landing weights for specific airports and runways; taking into account obstacle clearance, runway length and slope, aircraft configuration, and current meteorological conditions.
	CAT.POL. A.205/210/225
CAT.POL. A.310/315/330
CAT.POL. A.405/410/430

	
	
	
	

	2.9
	Conduct a review of Specific Approval (e.g. LVO, EFB, PBN, EDTO, RVSM, DG) and complete checklists for the new variant as applicable
	SPA.GEN.105
SPA.GEN.115
SPA.GEN.120
SPA.PBN.100
SPA.PBN.105
SPA.MNPS.100
SPA.MNPS.105
SPA.RVSM.100
SPA.RVSM.105
SPA.LVO.100
SPA.LVO.105
SPA.EDTO.100
SPA.EDTO.105
SPA.EDTO.110
SPA.EFB.100
	
	
	 
	

	3
	     Airworthiness (AW)
	
	
	
	
	
	

	3.1
	Has the GMM been revised to reflect the impact of the new type or variant of aircraft?
	ORO.GEN.110
ORO.MLR.100
	
	
	
	

	3.2
	Has the Maintenance Programme been revised to reflect the impact of the variant of aircraft, or a new AMP produced for the new type?   

For a new AMP review it using the AMP Checklist? 
	ORO.GEN.110
ORO.MLR.100
	
	
	
	

	3.3
	Has the reliability program been revised to reflect the variant of aircraft or new type? (if applicable)
	ORO.GEN.110
ORO.MLR.100
	
	
	
	

	3.4
	Has the engine condition monitoring program been revised to reflect the variant of aircraft or new type (if applicable)
	ORO.GEN.110
ORO.MLR.100
	
	
	
	

	3.5
	Has the ETOPS manual been revised to reflect the variant of aircraft or new type (if applicable)
	SPA.EDTO.100
SPA.EDTO.101
SPA.EDTO.105
SPA.EDTO.110
GM1 SPA.EDTO 
AMC1 SPA.EDTO.105
GM1 SPA.EDTO.105 & 110
AMC1 SPA.EDTO. 110
	
	
	
	

	3.6
	Have the aircraft records been updated to include the required records for the variant of aircraft or new type?
	ORO.GEN.110
ORO.MLR.100
	
	
	
	

	3.7
	Has the operator evaluated and arranged all technical documents from TC holder for variant of aircraft or new type such as IPC, AMM, SRM etc.
	ORO.GEN.110
ORO.MLR.100
	
	
	
	

	3.8
	Conduct a review of Specific Approval (e.g. LVO, EFB, PBN, EDTO, RVSM, DG) and complete checklists for the  variant of aircraft or new type (if applicable)

	SPA.GEN.105
SPA.GEN.115
SPA.GEN.120
SPA.PBN.100
SPA.PBN.105
SPA.MNPS.100
SPA.MNPS.105
SPA.RVSM.100
SPA.RVSM.105
SPA.LVO.100
SPA.LVO.105
SPA.EDTO.100
SPA.EDTO.105
SPA.EDTO.110
SPA.EFB.100
	
	
	
	
















	4
	Training (OPS and AW)
	
	
	
	
	

	4.1
	Has the operator established training required for differences between this aircraft variant and the existing AOC holder’s fleet of the type?
	ORO.FC.120
ORO.FC.125
ORO.FC.220
AMC1 ORO.FC.125
AMC2 ORO.FC.125
AMC1 ORO.FC.125(b)
AMC1 ORO.FC.220
AMC3 ORO.FC.220


	
	
	
	

	4.2
	For a new type or variant check, the appropriate training is addressed in the OM-D and Engineering manuals.
	ORO.FC.220

	
	
	
	

	5
	Sign off (OPS and AW)
	
	
	
	
	

	5.1
	Ops Sign off (POI): Name and Date 
	
	
	
	
	

	5.2
	AW Sign off (AWI): Name and Date 
	
	
	
	
	

	5.3
	OPS SPEC 
	
	
	
	
	



S = Satisfied
U= Unsatisfied   
N/A= Not Applicable
Comment= Description of the details of compliance or non-compliance or other information
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