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The CAMO Product Audit is made of 3 phases: The aircraft records review, the aircraft management system, and the aircraft physical inspection. 
The comment will be used to record sample subjects and collected evidence.
	[bookmark: _Hlk169187010]No
	Subject
	Reference
	S
	U
	N/A
	Comment

	
	PRODUCT INFORMATION
	
	
	
	
	

	
	Aircraft Type / Model / Series (Note: Use one checklist for one product line.)
	CAMO.A.135
CAMO.A.315
	
	
	
	

	
	Aircraft Registration Mark and MSN
	
	
	
	
	

	
	A/C TCDS No. and Rev.
	
	
	
	
	

	
	Engines Type
	
	
	
	
	

	
	ESN (#1, #2, #3, #4, …)
	
	
	
	
	

	
	Engines TCDS No. and Rev.
	
	
	
	
	

	
	Propellers Type
	
	
	
	
	

	
	PSN (#1, #2, #3, #4, …)
	
	
	
	
	

	
	Propellers TCDS No. and Rev.
	
	
	
	
	

	
	Aircraft Operator name
	
	
	
	
	

	
	Aircraft Operator Certificate’s number and validity (as applicable)
	
	
	
	
	

	
	Aircraft Operation Specifications (as applicable):
	
	
	
	
	

	
	No. and Rev.
	
	
	
	
	

	
	The aircraft type is listed in the AOC’s Operations Specifications.
	
	
	
	
	

	
	The aircraft registration is listed in the Attachment to Operations Specifications.
	
	
	
	
	

	
	Granted specific approvals
	
	
	
	
	

	
	Other active authorizations (Special Flight Permit, Operating license, etc.)
	
	
	
	
	

	
	C of R Issue Date
	
	
	
	
	

	
	C of A validity
	
	
	
	
	

	
	For leased aircraft, lease agreement validity:
	M.A.201
CAMO.A.135
ORO.AOC.110
ORO.AOC.115
	
	
	
	

	
	Ownership
	
	
	
	
	

	
	Period and duration
	
	
	
	
	

	
	Continuing airworthiness responsibility
	
	
	
	
	

	
	AIRCRAFT RECORDS REVIEW
	
	
	
	
	

	
	The aircraft complies with the latest approved type design:
	CAMO.A.315
	
	
	
	

	
	The aircraft, engines and propellers comply with the latest TCDS.
	
	
	
	
	

	
	The aircraft LOPA/ interior accommodation complies with approved configuration.
	
	
	
	
	

	
	Check the aircraft approved mass (MTOM, MLM, etc.)
	
	
	
	
	

	
	The aircraft, engines and propellers’ flight hours and cycles are properly recorded:
	CAMO.A.315
CAMO.A.220(a)
	
	
	
	

	
	Records reflect the status of the aircraft and hours/cycles are up to date.
	
	
	
	
	

	
	Review	hours/cycles up-date on ACARS, ATL (aircraft, engine, propeller, APU logbook).
	
	
	
	
	

	
	All maintenance due on the aircraft is accomplished in accordance with the approved maintenance program:
	CAMO.A.315
ORO.AOC.125
TCAR OPS Part SEA Subpart MCF
SPO.SPEC.MCF
NCO.SPEC.MCF
	
	
	
	

	
	Review the approval and update of the maintenance program.
	
	
	
	
	

	
	Sample that the aircraft maintenance records are in line with the content of the approved maintenance program.
	
	
	
	
	

	
	Check that the maintenance program is customised to the aircraft condition.
	
	
	
	
	

	
	Sample intervals between letter checks (A, C, D checks).
	
	
	
	
	

	
	Sample out-of-phases tasks accomplishment and intervals.
	
	
	
	
	

	
	Sample intervals between any extension and permitted variations.
	
	
	
	
	

	
	Sample accomplishment of maintenance tasks:
	
	
	
	
	

	
	Line maintenance task(s)
	
	
	
	
	

	
	Base maintenance task(s)
	
	
	
	
	

	
	Component replacement(s)
	
	
	
	
	

	
	Specialised maintenance task(s) e.g. NDT, painting, etc.
	
	
	
	
	

	
	Sample accomplishment of any maintenance deferrals.
	
	
	
	
	

	
	Sample life limited and time limited components status and change records.
	
	
	
	
	

	
	Sample airworthiness limitations and certification maintenance requirements.
	
	
	
	
	

	
	Sample accomplishment of any Maintenance Check Flight (MCF)
	
	
	
	
	

	
	All applicable ADs have been applied and recorded for airframe, engines, propeller, APU and appliances:
	CAMO.A.315
	
	
	
	

	
	Review	AD status vs State of Design issued AD’s and CAAT’s.
	
	
	
	
	

	
	For AD’s including repetitive inspections, sample the inclusion of these inspection requirements in the management system and the interval between inspections already accomplished.
	
	
	
	
	

	
	Sample AD evaluation and accomplishment records.
	
	
	
	
	

	
	For AMOC’s to AD’s, verify they are CAAT approved/accepted.
	
	
	
	
	

	
	All known defects have been properly rectified or carried forward:
	CAMO.A.315
ORO.MLR.105
SEA.MLR.105
NCO.GEN.155
	
	
	
	

	
	Review the current ‘Deferred/carried forward Defect’ list for open defects affecting aircraft operation.
	
	
	
	
	

	
	Sample that defects were deferred in accordance with CAAT approved maintenance data (MEL, AMM, CDL, DDG, etc.).
	
	
	
	
	

	
	Sample that defects are rectified within the delay/limits granted by the approved maintenance data.
	
	
	
	
	

	
	Control of any repetitive defects.
	
	
	
	
	

	
	All modifications applied are recorded and CAAT approved:
	CAMO.A.315

	
	
	
	

	
	Review SB’s and modifications status.
	
	
	
	
	

	
	Sample modifications files to ensure they are CAAT approved/accepted (STC, DOA, Part-21 approved modifications, etc.).
	
	
	
	
	

	
	Sample SB’s and modifications incorporation records.
	
	
	
	
	

	
	Sample of maintenance tasks introduced by modification including its documentation.
	
	
	
	
	

	
	All supplemental documents (Supplement AFM, MEL, AMM, IPC, ELA, ICA, etc.) are available and up to date.
	
	
	
	
	

	
	All repairs applied are recorded and CAAT approved/accepted.
	
	
	
	
	

	
	Review repair status (dent and buckle chart or damage marking).
	
	
	
	
	

	
	Sample repairs files to ensure they are CAAT approved/accepted (EO, Part 21 approved repairs, etc.).
	
	
	
	
	

	
	Sample repairs incorporation records.
	
	
	
	
	

	
	Sample repetitive maintenance task from repairs or allowable damages.
	
	
	
	
	

	
	Sample in-service limits from repairs or allowable damages.
	
	
	
	
	

	
	The current mass and balance statement reflects the aircraft configuration.
	CAMO.A.315
CAT.POL.MAB
SEA.CSO.MAB
SPO.POL.105
NCC.POL.105
NCO.POL.105
	
	
	
	

	
	Control that mass and balance report reflects the current aircraft configuration and is valid.
	
	
	
	
	

	
	Periodical aircraft weighing is accomplished in accordance with the operator’s policy/approved maintenance program.
	
	
	
	
	

	
	Control that aircraft weighing is done after modifications or repairs, as required.
	
	
	
	
	

	
	The mass and balance report are fully represented in aircraft prepared for service weights and indices used in the loading calculations made prior to flight dispatch.
	
	
	
	
	

	
	The maintenance is always released to service by CAAT approved maintenance organisations and recorded in aircraft continuing airworthiness record system and applicable aircraft technical log system.
	CAMO.A.220
CAMO.A.315
	
	
	
	

	
	Sample aircraft technical log system, aircraft logbook, engine logbooks, propeller logbooks, APU logbook entries and components release to services.
	
	
	
	
	

	
	Sample the use of release to service documentation (statement and required minimum information).
	
	
	
	
	

	
	The status of aircraft operational-derived equipment meets operational requirements:
	CAMO.A.315
CAT.GEN.MPA.195
CAT.IDE.A/H
SEA.CSO.IDE
ORO.AOC.105 
TCAR OPS Part-SPA
SPO.GEN.145
SPO.IDE.A/H
NCC.GEN.145
NCC.IDE.A/H
NCO.IDE.A/H
TCAR OPS Part-SPO Subpart SPEC
TCAR OPS Part-NCO Subpart SPEC
	
	
	
	

	
	Installation and tasks for instrument and equipment for operations, communication, navigation, and surveillance, including but not limited to:
1. Safety equipment (depends on the aircraft’s type of operation)
1. Flight recorders (including its documentation and recording inspections)
1. ELT coding and registration
1. Mode-S address field test
	
	
	
	
	

	
	Installation and maintenance for instrument/equipment/system for granted specific approvals or specialised operations or other authorizations.
	
	
	
	
	

	
	Control of electronic aeronautical database management, as applicable:
1. Navigation database
Terrain database
Other software application
	
	
	
	
	

	
	Control of lists containing information of the emergency and survival equipment carried on board.
	
	
	
	
	

	
	Accomplishment of pre-flight inspections
	CAMO.A.315
	
	
	
	

	
	As applicable, reliability report of this aircraft type including:
	CAMO.A.315
M.A.302(g)
	
	
	
	

	
	Management of dispatch reliability including delays and cancellations
	
	
	
	
	

	
	Management of systems and equipment failure rates
	
	
	
	
	

	
	Management of engine reliability, IFSD rate, and applicable EDTO capability
	
	
	
	
	

	
	Management of CAT II/III system reliability
	
	
	
	
	

	
	MANAGEMENT SYSTEM
	
	
	
	
	

	
	SMS
	
	
	
	
	

	
	Any safety finding relevant to this aircraft type has been identified with root cause and contributing factors to prevent reoccurrence.
	CAMO.A.160
CAMO.A.200(a)(1)
CAMO.A.202
CAMO.A.205
ORO.GEN.155
ORO.GEN.160
ORO.GEN.200
	
	
	
	

	
	Any safety measure/information mandated by CAAT relevant to this aircraft type has been effectively implemented.
	
	
	
	
	

	
	The mandatory occurrences relevant to selected aircraft registration are reported to the following entities, within 72 hours after being identified:
1. CAAT
Organisation responsible for the design of the aircraft
Organization responsible for engine or propeller type design, when related
Individual or organization responsible for the design of the modification or repair, when related
	
	
	
	
	

	
	The mandatory occurrence report and follow-up report for the selected aircraft registration are made in a form and manner established by CAAT with the required information.
	
	
	
	
	

	
	For occurrence of the selected aircraft registration, hazard and risk assessment have been carried out and/or investigated and mitigated.
	
	
	
	
	

	
	Any change to aircraft configuration (major modification/repair) for this aircraft type is managed i.a.w. Management of Change procedures.
	
	
	
	
	

	
	Any aviation safety hazards associated with any contracting or subcontracting of this aircraft type are considered as part of the organisation’s management system.
	
	
	
	
	

	
	COMPLIANCE MONITORING
	
	
	
	
	

	
	Sample product audit that is performed by quality function for this aircraft type.
	CAMO.A.200(a)(2)
	
	
	
	

	
	Any quality audit finding relevant to this aircraft type has been addressed and implemented with corrective actions.
	
	
	
	
	

	
	The following personnel competency for this aircraft type are controlled, trained, and their competency is assessed for the task they performed:
1. Nominated personnel
CAM personnel - Engineering and planning
CAM personnel - Reliability and engine monitoring
Quality audit personnel – Auditor
Airworthiness Review Staff (ARS)
Airworthiness Review Staff Examiner (ARSX)
	CAMO.A.200(a)(1)(iv)
CAMO.A.305
CAMO.A.310
	
	
	
	

	
	The subcontracted organisation who performs any subcontracted tasks for this aircraft type is covered and works under the operator’s management system:
1. Covered by the operator’s training program and competency control
1. Covered by operator’s audit program
1. Covered by operator’s SMS
1. Any changes affecting the contract are notified to the operator by the subcontracted organisation, then to CAAT by the operator
	CAMO.A.205
M(L).A.201
	
	
	
	

	
	The contract and subcontract organisations performing tasks for this aircraft type are valid and controlled.
	
	
	
	
	

	
	AIRWORTHINESS REVIEW
	
	
	
	
	

	
	Sample intervals between AR accomplishment.
	CAMO.A.320
	
	
	
	

	
	AR is carried out with full documented review of aircraft records and aircraft physical survey.
	
	
	
	
	

	
	The AR of the aircraft is performed by the authorized CMR staff.
	
	
	
	
	

	
	The AR report is issued only when the aircraft is airworthy.
	
	
	
	
	

	
	The AR task is not contracted or subcontracted.
	
	
	
	
	

	
	The AR report is submitted to CAAT within 10 days.
	
	
	
	
	

	
	AIRCRAFT PHYSICAL INSPECTION
	
	
	
	
	

	
	Aircraft exterior inspection, including but not limited to:
1. Nose	
Fuselage
Wing
Landing gear and wheel (and/or floats)
Engine including propeller if installed
Empennage / Tail
APU
	CAMO.A.315
	
	
	
	

	
	Cockpit inspection, including but not limited to:
1. Required on-board documents
1. Operational documents and instructions to flight crews
1. Cockpit doors and seats
1. Cockpit safety equipment
1. Cockpit displays and systems
1. Cockpit general condition
	CAMO.A.315
ORO.MLR.110
SEA.MLR.110
SPO.GEN.140
NCC.GEN.140
NCO.GEN.135
	
	
	
	

	
	Cabin/cargo inspection, including but not limited to:
1. Cabin interior configuration
Crew areas, galleys, rest area
Toilets / lavatory (if installed)
Passenger cabin
Cargo compartment	
	CAMO.A.315
	
	
	
	

	
	Operational-Derived Equipment (ODE) or system required for:
1. Instruments and equipment requirements
All granted specific approvals / specialised operations / other authorisations
	CAMO.A.315
	
	
	
	

	
	OVERALL
	
	
	
	
	

	
	Access to facility, aircraft, document, records, data, procedures or any other material relevant to its activity subject to certification for this aircraft type, whether it is contracted/ subcontracted or not, are provided to CAAT for determining compliance during this audit.
	CAMO.A.140
	
	
	
	

	
	The aircraft is maintained in accordance with CAAT Requirements in an airworthy condition under its applicable approval (AOC, OpSpec, Operating license, SFP, or other authorizations).
	CAMO.A.315
	
	
	
	

	
	The organisation performs activities on this aircraft type in accordance with their approved Terms of Approval, Privileges, and Scope of Work.
	CAMO.A.125
	
	
	
	



S = Satisfy, U= Unsatisfied, N/A= Not Applicable
Comment= Description the detail of compliance, Non-Compliance details, Reason for not-applicable, or other information

REMARKS:
	

	

	

	

	

	

	

	

	




	
	         Assessed by:   …………………………………………………
Inspector Name ( ……………………………………………….. )
                     Position …………………………………………..
                               Date ………………………………………….
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