	AIRWORTHINESS REVIEW REPORT for TCAR AIR PART-ML
CAAT FORM 15B 

	AIRWORTHINESS AND AIRCRAFT ENGINEERING DEPARTMENT


		[image: ]
	AR Entity (see Note 1)
	☐ CAMO       ☐ CAO       ☐ CAAT

	AR Entity Name
	
	Certificate No.
	

	AR Staff Name
	

	AR Staff Authorized No.
	

	Aircraft Operator Name
	

	Aircraft available at place and period:
(In case aircraft physical survey by CAAT is required)
	

	Notes for use: also refer to the Explanatory Notes at the end of this report
· Where an item is satisfactory, indicate ‘Y’ into the appropriate column. 
If not applicable, indicate ‘N/A’
· All aircraft defects will require maintenance action prior to further flight
	
	

	
	Date next review due
	

	
	One year after completed sign on Section 4 or 5

	· Section 5 cannot be certified if there is evidence or indications that the aircraft is not airworthy
· The Explanatory Notes’ pages are not required to be kept with the completed certified report 
· Send the report form to airworthiness@caat.or.th

	

	1. AIRCRAFT DETAILS

	Registration Mark 
(Or reserved mark for imported Aircraft)
	
	Previous Registration 
(Imported Aircraft)
	

	
	Airframe
	Engine(s) / Propulsion
	Propeller(s)

	Manufacturer
	
	
	

	Type / Model
	
	
	

	Serial No.
	
	#1
	#2

	#1

	#2

	Date of Manufacture
	
	#1

	#2

	#1

	#2


	Hours since new
	
	#1

	#2

	#1

	#2


	Cycles sine new
	
	#1

	#2

	#1

	#2


	State of Design
	
	
	

	State of Manufacture
	
	
	

	TCDS No.
	
	Rev.
	
	
	Rev.
	
	
	Rev.
	

	TCDS No. for Noise and Emissions
(For imported aircraft only)
	
	Rev.
	

	Maximum Take-Off Weight


		
	kg.

		

		

	2. DOCUMENT REVIEW

	Date of Document Review
	

	Place of Document Review
	

	C of R Reference
	
	C of R Issue Date
	

	C of A Reference
(or Export C of A for imported aircraft)
	
	C of A Expiry Date
(or Export C of A, as applicable)
	

	Airframe, engine and propeller flying hours and cycles have been properly recorded?
	

	The flight manual is applicable to the aircraft configuration and reflects the latest revision status?
	

	The maintenance programme in used reflects the latest revision of the OEM’s programme?
	

	All maintenance due according to the approved/declared maintenance program has been carried out?
	

	All known defects have been corrected or deferred in a controlled manner?
	

	All applicable Airworthiness Directives (AD) have been applied and properly registered?
	

	All modifications, and repairs made to the aircraft have been registered, approved/accepted by CAAT, and in compliance with approved design? 
	

	All time controlled and life limited components installed on the aircraft are properly identified, registered, and controlled in accordance with approved/declared maintenance program, 
and have not exceeded their mandatory limit?
	

	All maintenance has been certified and released in accordance with TCAR AIR Part-ML? 
	

	The current mass and balance statement reflect the current aircraft configuration and is valid?
	

	The aircraft holds a noise certificate corresponding to the current aircraft configuration?
	

	The aircraft complies with the latest revision of its type designed approved or validated by CAAT?
	

	List of persons or organizations having carried out continuing airworthiness activities including maintenance tasks on the aircraft and its component since the last airworthiness review:

	

	3. AIRCRAFT PHYSICAL SURVEY (see Note 2)

	Date of Aircraft Physical Survey
	

	Place of Aircraft Physical Survey
	

	Name of Assisting TCAR PEL Part-66 Personnel
(see Note 3)
	  The AR staff is also holding a valid licence
  Assisting Name: ___________________________

	Assisting TCAR PEL Part-66 Personnel’s Signature
	

	Licence No.
	
	Licence Valid Until
	

	The required documents to be on board are present?
	

	All required markings and placards (see Note 4) are properly installed and legible?
	

	The aircraft complies with its approved/accepted flight manual?
	

	The aircraft configuration complies with the approved documentation (TCDS, STC, etc.)?
	

	All defects have been correctly rectified or deferred in a controlled manner 
(No evidence defect that has not been addressed is found)?
	

	The aircraft condition is consistent with the documented review of records in Section 2 of this report?  
	

	


	

	4. DEFECTS / FINDINGS OBSERVED (see Note 5)
(All defects / findings must be cleared before certifying the review)

	Reference
	Defects / Findings Description
	Rectification / Actions

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	Extra page(s) attached ?  ______

	

	If the defects / findings have not been rectified by the report issuance date, the Airworthiness Review Staff may sign off on the report in this section. 
However, if the unresolved defects / findings endanger  flight safety, the aircraft must not be operated in accordance with ML.A.902(b).
	

________________________

(                                                               )

Report date:            /             /        

	

	

	5. CERTIFICATION (see Note 6)
(The review cannot be certified with open defects / findings)

	Statement

	I certify that all of the above records have been reviewed for the period plus a physical survey of the aircraft undertaken and the aircraft with the registration mark [ HS -              ] is found to be fully in compliance with all of the applicable requirements.

The aircraft in its current configuration complies with the following:
· Airworthiness directives up to the latest published issue
· Type certificate datasheet
· Maintenance programme
· Limitation for life-limited parts and time-controlled components
· The valid weight and center of gravity schedule reflecting the current configuration of the aircraft
· All modifications and repairs requirements
· The current flight manual including supplements
· Operational requirements

In addition, all of the above items are properly entered and certified in the aircraft continuing airworthiness record system and/or in its technical log.

At the time of the review, the aircraft is considered AIRWORTHY and complied with TCAR AIR Part-ML.


	Airworthiness Review Staff Signature
	I confirm that information in this report is true and accurate


________                                ________

(                                                               )

Report completed date:            /             /        .




Explanatory notes for completing the Airworthiness Review Report

General, for all sections
· Enter a ‘Y’ in the appropriate column to indicate that the aircraft meets the applicable requirements
· Enter ‘N/A’ if the requirement is not applicable to the aircraft or operation

Note 1
ML.A.901, GM1 ML.A.901
The airworthiness review and the issuance of the Airworthiness review report shall be performed in accordance with point ML.A.903, either by:
(1) in case of continuing airworthiness of aircraft is not managed by CAMO or CAO
a. an appropriately approved CAMO or CAO; or
b. CAAT;
(2) in case of continuing airworthiness of aircraft is managed by CAMO or CAO, the CAMO or CAO managing the continuing airworthiness of the aircraft.
If a CAMO/CAO holding the AR privilege is contracted by the owner, this organisation does not have the obligation to carry out the AR itself. The owner may select another CAMO or CAO to carry out the AR.
The list of the organisations or persons that are allowed to perform an AR does not presume that they have the obligation to accept a request to carry out an AR.
The “AR Entity Name” and “Certificate No.” data fields only applicable to CAMO, CAO, or AMO. For TCAR PEL Part-66 Personnel, fulfilling “AR Staff”, “AR Staff Authorized No.”, and “Licence No.” are sufficient.

Note 2
ML.A.903(c)
The physical survey could require actions categorised as maintenance (e.g. operational tests, tests of emergency equipment, visual inspections requiring panel opening, etc.). In this case, after the airworthiness review, a release to service should be issued. The physical survey may include verifications to be carried out during flight. To ensure compliance, the physical survey may include relevant sample checks of items.

Note 3
ML.A.903(b)
If the Airworthiness Review (AR) staff are qualified as TCAR PEL Part-66 personnel, fill in the licence number and validity.

When the AR staff are not appropriately qualified as TCAR PEL Part-66 personnel, in order to release any maintenance as recommended in Note 2, it is required them to be assisted by such qualified personnel. However, the function of such personnel is limited to performing and releasing the maintenance actions requested by the AR staff, it not being their function to perform the physical survey of the aircraft. This means that the AR staff who is going to sign the airworthiness review report should be the one performing both the documented review and the physical survey of the aircraft. It is not the intent of the rule to delegate the survey to TCAR PEL Part-66 personnel who are not AR staff.


Note 4
ML.A.903(c)(1)
The markings and placards can be required by certification information in the TCDS, the AFM, manufacturer instructions (ATA Chapter 11), the STCs’ ICA, ADs, or supplemental information from approved drawing/document.

Note 5
ML.A.903(e)
New aircraft defects identified during the review must also be recorded in the technical log by appropriate TCAR PEL Part-66 personnel. All aircraft defects require a clearing maintenance action (correction or deferral) prior to further flight.
As applicable to aircraft operator/owner who is required to develop their own customized Aircraft Maintenance Programme (AMP), when the effectiveness of the AMP is reviewed in conjunction with the airworthiness review in accordance with point (c)(9) of point ML.A.302 by the AR staff, if the review shows deficiencies of the aircraft linked with deficiencies in the content of the AMP, the AMP shall be amended accordingly. 
The person performing the review shall inform CAAT (via airworthiness@caat.or.th) if they do not agree with the measures amending the AMP taken by the owner, CAMO or CAO. In such case CAAT will decide which amendments to the AMP are necessary, raising the corresponding findings and, if necessary, suspend or revoke the certificate of airworthiness.
In case of the defects / findings have not been rectified by the report issuance date, the next review due date shall be calculated from the completion date in Section 4 of this report.

Note 6
ML.A.903(f)
THE REPORT CANNOT BE CERTIFIED WITH OPEN FINDINGS. Each finding requires a corrective action before the certification of the ARR. The corrective action should be adequate to the open finding and it should be carried out and verified by the AR staff before the issue of the ARR.
Once the report is completed and certified, it should be kept along with the documents listed at the end of Section 2 of this report including all reviewed documents. The copy of airworthiness review must be available for CAAT upon request.
Once the report is completed and certified, it must be submitted to airworthiness@caat.or.th within 10 days.
The next review due date shall be calculated from the certification date in Section 5 of this report.
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